;DUCT_DIAMETER##HVAC_DUCT_SIZE##MILLIMETERS;Nominal dimension##LENGTH##MILLIMETERS;Number of vanes##LENGTH##MILLIMETERS;Description##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;Model##OTHER##;URL##OTHER##;Front panel##OTHER##;Front panel square##OTHER##;Upper connection##OTHER##
VVM 300 C/V/P/8;160;300;8;Anemostat;square front panel, 300mm, horizontal connection, number of vanes 8, air supply, without regulating flap;MANDÍK;VVM 300 C/V/P/8;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 300 C/V/P/8/R;160;300;8;Anemostat;square front panel, 300mm, horizontal connection, number of vanes 8, air supply, with regulating flap;MANDÍK;VVM 300 C/V/P/8/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 300 C/S/P/8;160;300;8;Anemostat;square front panel, 300mm, vertical connection, number of vanes 8, air supply, without regulating flap;MANDÍK;VVM 300 C/S/P/8;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 300 C/S/P/8/R;160;300;8;Anemostat;square front panel, 300mm, vertical connection, number of vanes 8, air supply, with regulating flap;MANDÍK;VVM 300 C/S/P/8/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 400 C/V/P/16;200;400;16;Anemostat;square front panel, 400mm, horizontal connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 400 C/V/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 400 C/V/P/16/R;200;400;16;Anemostat;square front panel, 400mm, horizontal connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 400 C/V/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 400 C/S/P/16;200;400;16;Anemostat;square front panel, 400mm, vertical connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 400 C/S/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 400 C/S/P/16/R;200;400;16;Anemostat;square front panel, 400mm, vertical connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 400 C/S/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 500 C/V/P/16;200;500;16;Anemostat;square front panel, 500mm, horizontal connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 500 C/V/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 500 C/V/P/24;200;500;24;Anemostat;square front panel, 500mm, horizontal connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 500 C/V/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 500 C/V/P/16/R;200;500;16;Anemostat;square front panel, 500mm, horizontal connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 500 C/V/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 500 C/V/P/24/R;200;500;24;Anemostat;square front panel, 500mm, horizontal connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 500 C/V/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 500 C/S/P/16;200;500;16;Anemostat;square front panel, 500mm, vertical connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 500 C/S/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 500 C/S/P/24;200;500;24;Anemostat;square front panel, 500mm, vertical connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 500 C/S/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 500 C/S/P/16/R;200;500;16;Anemostat;square front panel, 500mm, vertical connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 500 C/S/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 500 C/S/P/24/R;200;500;24;Anemostat;square front panel, 500mm, vertical connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 500 C/S/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 600 C/V/P/16;200;600;16;Anemostat;square front panel, 600mm, horizontal connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 600 C/V/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 600 C/V/P/24;250;600;24;Anemostat;square front panel, 600mm, horizontal connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 600 C/V/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 600 C/V/P/48;250;600;48;Anemostat;square front panel, 600mm, horizontal connection, number of vanes 48, air supply, without regulating flap;MANDÍK;VVM 600 C/V/P/48;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 600 C/V/P/16/R;200;600;16;Anemostat;square front panel, 600mm, horizontal connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 600 C/V/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 600 C/V/P/24/R;250;600;24;Anemostat;square front panel, 600mm, horizontal connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 600 C/V/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 600 C/V/P/48/R;250;600;48;Anemostat;square front panel, 600mm, horizontal connection, number of vanes 48, air supply, with regulating flap;MANDÍK;VVM 600 C/V/P/48/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 600 C/S/P/16;200;600;16;Anemostat;square front panel, 600mm, vertical connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 600 C/S/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 600 C/S/P/24;250;600;24;Anemostat;square front panel, 600mm, vertical connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 600 C/S/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 600 C/S/P/48;250;600;48;Anemostat;square front panel, 600mm, vertical connection, number of vanes 48, air supply, without regulating flap;MANDÍK;VVM 600 C/S/P/48;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 600 C/S/P/16/R;200;600;16;Anemostat;square front panel, 600mm, vertical connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 600 C/S/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 600 C/S/P/24/R;250;600;24;Anemostat;square front panel, 600mm, vertical connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 600 C/S/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 600 C/S/P/48/R;250;600;48;Anemostat;square front panel, 600mm, vertical connection, number of vanes 48, air supply, with regulating flap;MANDÍK;VVM 600 C/S/P/48/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 625 C/V/P/16;200;625;16;Anemostat;square front panel, 625mm, horizontal connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 625 C/V/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 625 C/V/P/24;250;625;24;Anemostat;square front panel, 625mm, horizontal connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 625 C/V/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 625 C/V/P/48;250;625;48;Anemostat;square front panel, 625mm, horizontal connection, number of vanes 48, air supply, without regulating flap;MANDÍK;VVM 625 C/V/P/48;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 625 C/V/P/16/R;200;625;16;Anemostat;square front panel, 625mm, horizontal connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 625 C/V/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 625 C/V/P/24/R;250;625;24;Anemostat;square front panel, 625mm, horizontal connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 625 C/V/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 625 C/V/P/48/R;250;625;48;Anemostat;square front panel, 625mm, horizontal connection, number of vanes 48, air supply, with regulating flap;MANDÍK;VVM 625 C/V/P/48/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 625 C/S/P/16;200;625;16;Anemostat;square front panel, 625mm, vertical connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 625 C/S/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 625 C/S/P/24;250;625;24;Anemostat;square front panel, 625mm, vertical connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 625 C/S/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 625 C/S/P/48;250;625;48;Anemostat;square front panel, 625mm, vertical connection, number of vanes 48, air supply, without regulating flap;MANDÍK;VVM 625 C/S/P/48;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 625 C/S/P/16/R;200;625;16;Anemostat;square front panel, 625mm, vertical connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 625 C/S/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 625 C/S/P/24/R;250;625;24;Anemostat;square front panel, 625mm, vertical connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 625 C/S/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 625 C/S/P/48/R;250;625;48;Anemostat;square front panel, 625mm, vertical connection, number of vanes 48, air supply, with regulating flap;MANDÍK;VVM 625 C/S/P/48/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 825 C/V/P/72;315;825;72;Anemostat;square front panel, 825mm, horizontal connection, number of vanes 72, air supply, without regulating flap;MANDÍK;VVM 825 C/V/P/72;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 825 C/V/P/72/R;315;825;72;Anemostat;square front panel, 825mm, horizontal connection, number of vanes 72, air supply, with regulating flap;MANDÍK;VVM 825 C/V/P/72/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;0
VVM 825 C/S/P/72;315;825;72;Anemostat;square front panel, 825mm, vertical connection, number of vanes 72, air supply, without regulating flap;MANDÍK;VVM 825 C/S/P/72;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 825 C/S/P/72/R;315;825;72;Anemostat;square front panel, 825mm, vertical connection, number of vanes 72, air supply, with regulating flap;MANDÍK;VVM 825 C/S/P/72/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;1;1
VVM 300 C/8 fp supply;160;300;8;Anemostat;square front panel, 300mm, number of vanes 8, without regulating flap;MANDÍK;VVM 300 C/8 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;1;1
VVM 400 C/16 fp supply;200;400;16;Anemostat;square front panel, 400mm, number of vanes 16, without regulating flap;MANDÍK;VVM 400 C/16 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;1;1
VVM 500 C/16 fp supply;200;500;16;Anemostat;square front panel, 500mm, number of vanes 16, without regulating flap;MANDÍK;VVM 500 C/16 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;1;1
VVM 600 C/16 fp supply;200;600;16;Anemostat;square front panel, 600mm, number of vanes 16, without regulating flap;MANDÍK;VVM 600 C/16 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;1;1
VVM 625 C/16 fp supply;200;625;16;Anemostat;square front panel, 625mm, number of vanes 16, without regulating flap;MANDÍK;VVM 625 C/16 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;1;1
VVM 500 C/24 fp supply;200;500;24;Anemostat;square front panel, 500mm, number of vanes 24, without regulating flap;MANDÍK;VVM 500 C/24 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;1;1
VVM 600 C/24 fp supply;250;600;24;Anemostat;square front panel, 600mm, number of vanes 24, without regulating flap;MANDÍK;VVM 600 C/24 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;1;1
VVM 625 C/24 fp supply;250;625;24;Anemostat;square front panel, 625mm, number of vanes 24, without regulating flap;MANDÍK;VVM 625 C/24 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;1;1
VVM 600 C/48 fp supply;250;600;48;Anemostat;square front panel, 600mm, number of vanes 48, without regulating flap;MANDÍK;VVM 600 C/48 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;1;1
VVM 625 C/48 fp supply;250;625;48;Anemostat;square front panel, 625mm, number of vanes 48, without regulating flap;MANDÍK;VVM 625 C/48 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;1;1
VVM 825 C/72 fp supply;315;825;72;Anemostat;square front panel, 825mm, number of vanes 72, without regulating flap;MANDÍK;VVM 825 C/72 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;1;1
VVM 300 K/V/P/8;160;300;8;Anemostat;round front panel, 300mm, horizontal connection, number of vanes 8, air supply, without regulating flap;MANDÍK;VVM 300 K/V/P/8;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 300 K/V/P/8/R;160;300;8;Anemostat;round front panel, 300mm, horizontal connection, number of vanes 8, air supply, with regulating flap;MANDÍK;VVM 300 K/V/P/8/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 300 K/S/P/8;160;300;8;Anemostat;round front panel, 300mm, vertical connection, number of vanes 8, air supply, without regulating flap;MANDÍK;VVM 300 K/S/P/8;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 300 K/S/P/8/R;160;300;8;Anemostat;round front panel, 300mm, vertical connection, number of vanes 8, air supply, with regulating flap;MANDÍK;VVM 300 K/S/P/8/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 400 K/V/P/16;200;400;16;Anemostat;round front panel, 400mm, horizontal connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 400 K/V/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 400 K/V/P/16/R;200;400;16;Anemostat;round front panel, 400mm, horizontal connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 400 K/V/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 400 K/S/P/16;200;400;16;Anemostat;round front panel, 400mm, vertical connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 400 K/S/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 400 K/S/P/16/R;200;400;16;Anemostat;round front panel, 400mm, vertical connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 400 K/S/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 500 K/V/P/16;200;500;16;Anemostat;round front panel, 500mm, horizontal connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 500 K/V/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 500 K/V/P/24;200;500;24;Anemostat;round front panel, 500mm, horizontal connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 500 K/V/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 500 K/V/P/16/R;200;500;16;Anemostat;round front panel, 500mm, horizontal connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 500 K/V/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 500 K/V/P/24/R;200;500;24;Anemostat;round front panel, 500mm, horizontal connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 500 K/V/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 500 K/S/P/16;200;500;16;Anemostat;round front panel, 500mm, vertical connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 500 K/S/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 500 K/S/P/24;200;500;24;Anemostat;round front panel, 500mm, vertical connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 500 K/S/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 500 K/S/P/16/R;200;500;16;Anemostat;round front panel, 500mm, vertical connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 500 K/S/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 500 K/S/P/24/R;200;500;24;Anemostat;round front panel, 500mm, vertical connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 500 K/S/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 600 K/V/P/16;200;600;16;Anemostat;round front panel, 600mm, horizontal connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 600 K/V/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 600 K/V/P/24;250;600;24;Anemostat;round front panel, 600mm, horizontal connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 600 K/V/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 600 K/V/P/48;250;600;48;Anemostat;round front panel, 600mm, horizontal connection, number of vanes 48, air supply, without regulating flap;MANDÍK;VVM 600 K/V/P/48;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 600 K/V/P/16/R;200;600;16;Anemostat;round front panel, 600mm, horizontal connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 600 K/V/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 600 K/V/P/24/R;250;600;24;Anemostat;round front panel, 600mm, horizontal connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 600 K/V/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 600 K/V/P/48/R;250;600;48;Anemostat;round front panel, 600mm, horizontal connection, number of vanes 48, air supply, with regulating flap;MANDÍK;VVM 600 K/V/P/48/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 600 K/S/P/16;200;600;16;Anemostat;round front panel, 600mm, vertical connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 600 K/S/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 600 K/S/P/24;250;600;24;Anemostat;round front panel, 600mm, vertical connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 600 K/S/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 600 K/S/P/48;250;600;48;Anemostat;round front panel, 600mm, vertical connection, number of vanes 48, air supply, without regulating flap;MANDÍK;VVM 600 K/S/P/48;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 600 K/S/P/16/R;200;600;16;Anemostat;round front panel, 600mm, vertical connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 600 K/S/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 600 K/S/P/24/R;250;600;24;Anemostat;round front panel, 600mm, vertical connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 600 K/S/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 600 K/S/P/48/R;250;600;48;Anemostat;round front panel, 600mm, vertical connection, number of vanes 48, air supply, with regulating flap;MANDÍK;VVM 600 K/S/P/48/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 625 K/V/P/16;200;625;16;Anemostat;round front panel, 625mm, horizontal connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 625 K/V/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 625 K/V/P/24;250;625;24;Anemostat;round front panel, 625mm, horizontal connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 625 K/V/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 625 K/V/P/48;250;625;48;Anemostat;round front panel, 625mm, horizontal connection, number of vanes 48, air supply, without regulating flap;MANDÍK;VVM 625 K/V/P/48;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 625 K/V/P/16/R;200;625;16;Anemostat;round front panel, 625mm, horizontal connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 625 K/V/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 625 K/V/P/24/R;250;625;24;Anemostat;round front panel, 625mm, horizontal connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 625 K/V/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 625 K/V/P/48/R;250;625;48;Anemostat;round front panel, 625mm, horizontal connection, number of vanes 48, air supply, with regulating flap;MANDÍK;VVM 625 K/V/P/48/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 625 K/S/P/16;200;625;16;Anemostat;round front panel, 625mm, vertical connection, number of vanes 16, air supply, without regulating flap;MANDÍK;VVM 625 K/S/P/16;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 625 K/S/P/24;250;625;24;Anemostat;round front panel, 625mm, vertical connection, number of vanes 24, air supply, without regulating flap;MANDÍK;VVM 625 K/S/P/24;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 625 K/S/P/48;250;625;48;Anemostat;round front panel, 625mm, vertical connection, number of vanes 48, air supply, without regulating flap;MANDÍK;VVM 625 K/S/P/48;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 625 K/S/P/16/R;200;625;16;Anemostat;round front panel, 625mm, vertical connection, number of vanes 16, air supply, with regulating flap;MANDÍK;VVM 625 K/S/P/16/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 625 K/S/P/24/R;250;625;24;Anemostat;round front panel, 625mm, vertical connection, number of vanes 24, air supply, with regulating flap;MANDÍK;VVM 625 K/S/P/24/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 625 K/S/P/48/R;250;625;48;Anemostat;round front panel, 625mm, vertical connection, number of vanes 48, air supply, with regulating flap;MANDÍK;VVM 625 K/S/P/48/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 825 K/V/P/72;315;825;72;Anemostat;round front panel, 825mm, horizontal connection, number of vanes 72, air supply, without regulating flap;MANDÍK;VVM 825 K/V/P/72;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 825 K/V/P/72/R;315;825;72;Anemostat;round front panel, 825mm, horizontal connection, number of vanes 72, air supply, with regulating flap;MANDÍK;VVM 825 K/V/P/72/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;0
VVM 825 K/S/P/72;315;825;72;Anemostat;round front panel, 825mm, vertical connection, number of vanes 72, air supply, without regulating flap;MANDÍK;VVM 825 K/S/P/72;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 825 K/S/P/72/R;315;825;72;Anemostat;round front panel, 825mm, vertical connection, number of vanes 72, air supply, with regulating flap;MANDÍK;VVM 825 K/S/P/72/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;0;0;1
VVM 300 K/8 fp supply;160;300;8;Anemostat;round front panel, 300mm, number of vanes 8, without regulating flap;MANDÍK;VVM 300 K/8 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;0;1
VVM 400 K/16 fp supply;200;400;16;Anemostat;round front panel, 400mm, number of vanes 16, without regulating flap;MANDÍK;VVM 400 K/16 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;0;1
VVM 500 K/16 fp supply;200;500;16;Anemostat;round front panel, 500mm, number of vanes 16, without regulating flap;MANDÍK;VVM 500 K/16 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;0;1
VVM 600 K/16 fp supply;200;600;16;Anemostat;round front panel, 600mm, number of vanes 16, without regulating flap;MANDÍK;VVM 600 K/16 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;0;1
VVM 625 K/16 fp supply;200;625;16;Anemostat;round front panel, 625mm, number of vanes 16, without regulating flap;MANDÍK;VVM 625 K/16 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;0;1
VVM 500 K/24 fp supply;200;500;24;Anemostat;round front panel, 500mm, number of vanes 24, without regulating flap;MANDÍK;VVM 500 K/24 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;0;1
VVM 600 K/24 fp supply;250;600;24;Anemostat;round front panel, 600mm, number of vanes 24, without regulating flap;MANDÍK;VVM 600 K/24 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;0;1
VVM 625 K/24 fp supply;250;625;24;Anemostat;round front panel, 625mm, number of vanes 24, without regulating flap;MANDÍK;VVM 625 K/24 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;0;1
VVM 600 K/48 fp supply;250;600;48;Anemostat;round front panel, 600mm, number of vanes 48, without regulating flap;MANDÍK;VVM 600 K/48 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;0;1
VVM 625 K/48 fp supply;250;625;48;Anemostat;round front panel, 625mm, number of vanes 48, without regulating flap;MANDÍK;VVM 625 K/48 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;0;1
VVM 825 K/72 fp supply;315;825;72;Anemostat;round front panel, 825mm, number of vanes 72, without regulating flap;MANDÍK;VVM 825 K/72 fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvm;1;0;1
