;Number of outlets##OTHER##;Description##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;Model##OTHER##;URL##OTHER##
VAPM-L 2;2;Anemostat;without dispersion feature, screw hole without countersunk indentation, size 2;MANDÍK;VAPM-L 2;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 2 P;2;Anemostat;with dispersion feature, screw hole without countersunk indentation, size 2;MANDÍK;VAPM-L 2 P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 2 O;2;Anemostat;without dispersion feature, countersunk screw indentation in front panel, size 2;MANDÍK;VAPM-L 2 O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 2 O/P;2;Anemostat;with dispersion feature, countersunk screw indentation in front panel, size 2;MANDÍK;VAPM-L 2 O/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 3;3;Anemostat;without dispersion feature, screw hole without countersunk indentation, size 3;MANDÍK;VAPM-L 3;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 3 P;3;Anemostat;with dispersion feature, screw hole without countersunk indentation, size 3;MANDÍK;VAPM-L 3 P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 3 O;3;Anemostat;without dispersion feature, countersunk screw indentation in front panel, size 3;MANDÍK;VAPM-L 3 O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 3 O/P;3;Anemostat;with dispersion feature, countersunk screw indentation in front panel, size 3;MANDÍK;VAPM-L 3 O/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 4;4;Anemostat;without dispersion feature, screw hole without countersunk indentation, size 4;MANDÍK;VAPM-L 4;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 4  P;4;Anemostat;with dispersion feature, screw hole without countersunk indentation, size 4;MANDÍK;VAPM-L 4  P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 4 O;4;Anemostat;without dispersion feature, countersunk screw indentation in front panel, size 4;MANDÍK;VAPM-L 4 O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 4 O/P;4;Anemostat;with dispersion feature, countersunk screw indentation in front panel, size 4;MANDÍK;VAPM-L 4 O/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 5;5;Anemostat;without dispersion feature, screw hole without countersunk indentation, size 5;MANDÍK;VAPM-L 5;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 5 P;5;Anemostat;with dispersion feature, screw hole without countersunk indentation, size 5;MANDÍK;VAPM-L 5 P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 5 O;5;Anemostat;without dispersion feature, countersunk screw indentation in front panel, size 5;MANDÍK;VAPM-L 5 O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 5 O/P;5;Anemostat;with dispersion feature, countersunk screw indentation in front panel, size 5;MANDÍK;VAPM-L 5 O/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 6;6;Anemostat;without dispersion feature, screw hole without countersunk indentation, size 6;MANDÍK;VAPM-L 6;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 6 P;6;Anemostat;with dispersion feature, screw hole without countersunk indentation, size 6;MANDÍK;VAPM-L 6 P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 6 O;6;Anemostat;without dispersion feature, countersunk screw indentation in front panel, size 6;MANDÍK;VAPM-L 6 O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
VAPM-L 6 O/P;6;Anemostat;with dispersion feature, countersunk screw indentation in front panel, size 6;MANDÍK;VAPM-L 6 O/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm-l
