;Nominal dimension##LENGTH##MILLIMETERS;Description##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;Model##OTHER##;URL##OTHER##;Upper connection##OTHER##;Side connection##OTHER##;Front panel##OTHER##
ALKM 400 S/O/R;400;Anemostat;vertical connection, 400mm, with regulating flap, air exhaust;MANDÍK;ALKM 400 S/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;1;0;0
ALKM 500 V/O;500;Anemostat;vertical connection, 500mm, without regulating flap, air exhaust;MANDÍK;ALKM 500 V/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;0
ALKM 500 V/O/R;500;Anemostat;vertical connection, 500mm, with regulating flap, air exhaust;MANDÍK;ALKM 500 V/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;0
ALKM 500 S/O;500;Anemostat;vertical connection, 500mm, without regulating flap, air exhaust;MANDÍK;ALKM 500 S/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;1;0;0
ALKM 500 S/O/R;500;Anemostat;vertical connection, 500mm, with regulating flap, air exhaust;MANDÍK;ALKM 500 S/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;1;0;0
ALKM 600 V/O;600;Anemostat;vertical connection, 600mm, without regulating flap, air exhaust;MANDÍK;ALKM 600 V/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;0
ALKM 600 V/O/R;600;Anemostat;vertical connection, 600mm, with regulating flap, air exhaust;MANDÍK;ALKM 600 V/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;0
ALKM 600 S/O;600;Anemostat;vertical connection, 600mm, without regulating flap, air exhaust;MANDÍK;ALKM 600 S/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;1;0;0
ALKM 600 S/O/R;600;Anemostat;vertical connection, 600mm, with regulating flap, air exhaust;MANDÍK;ALKM 600 S/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;1;0;0
ALKM 250 fp exhaust;250;Anemostat;front panel, 250mm, without regulating flap;MANDÍK;ALKM 250 fp exhaust;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;1
ALKM 300 fp exhaust;300;Anemostat;front panel, 300mm, without regulating flap;MANDÍK;ALKM 300 fp exhaust;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;1
ALKM 400 fp exhaust;400;Anemostat;front panel, 400mm, without regulating flap;MANDÍK;ALKM 400 fp exhaust;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;1
ALKM 500 fp exhaust;500;Anemostat;front panel, 500mm, without regulating flap;MANDÍK;ALKM 500 fp exhaust;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;1
ALKM 600 fp exhaust;600;Anemostat;front panel, 600mm, without regulating flap;MANDÍK;ALKM 600 fp exhaust;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;1
ALKM 400 S/O;400;Anemostat;vertical connection, 400mm, without regulating flap, air exhaust;MANDÍK;ALKM 400 S/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;1;0;0
ALKM 400 V/O/R;400;Anemostat;vertical connection, 400mm, with regulating flap, air exhaust;MANDÍK;ALKM 400 V/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;0
ALKM 400 V/O;400;Anemostat;vertical connection, 400mm, without regulating flap, air exhaust;MANDÍK;ALKM 400 V/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;0
ALKM 300 S/O/R;300;Anemostat;vertical connection, 300mm, with regulating flap, air exhaust;MANDÍK;ALKM 300 S/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;1;0;0
ALKM 300 S/O;300;Anemostat;vertical connection, 300mm, without regulating flap, air exhaust;MANDÍK;ALKM 300 S/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;1;0;0
ALKM 300 V/O/R;300;Anemostat;vertical connection, 300mm, with regulating flap, air exhaust;MANDÍK;ALKM 300 V/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;0
ALKM 300 V/O;300;Anemostat;vertical connection, 300mm, without regulating flap, air exhaust;MANDÍK;ALKM 300 V/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;0
ALKM 250 S/O/R;250;Anemostat;vertical connection, 250mm, with regulating flap, air exhaust;MANDÍK;ALKM 250 S/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;1;0;0
ALKM 250 S/O;250;Anemostat;vertical connection, 250mm, without regulating flap, air exhaust;MANDÍK;ALKM 250 S/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;1;0;0
ALKM 250 V/O/R;250;Anemostat;vertical connection, 250mm, with regulating flap, air exhaust;MANDÍK;ALKM 250 V/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;0
ALKM 250 V/O;250;Anemostat;vertical connection, 250mm, without regulating flap, air exhaust;MANDÍK;ALKM 250 V/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/alkm;0;1;0
