;Nominal dimension##LENGTH##MILLIMETERS;DUCT_DIAMETER##HVAC_DUCT_SIZE##MILLIMETERS;Description##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;Model##OTHER##;URL##OTHER##;Front panel##OTHER##;Upper connection##OTHER##;Square front panel##OTHER##
VVPM 300/K/V/P;300;160;Anemostat;round front panel, 300mm,  horizontal connection, air supply, without regulating flap;MANDÍK;VVPM 300/K/V/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;0
VVPM 300/K/V/P/R;300;160;Anemostat;round front panel, 300mm,  horizontal connection, air supply, with regulating flap;MANDÍK;VVPM 300/K/V/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;0
VVPM 300/K/S/P;300;160;Anemostat;round front panel, 300mm,  vertical connection, air supply, without regulating flap;MANDÍK;VVPM 300/K/S/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;0
VVPM 300/K/S/P/R;300;160;Anemostat;round front panel, 300mm,  vertical connection, air supply, with regulating flap;MANDÍK;VVPM 300/K/S/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;0
VVPM 400/K/V/P;400;200;Anemostat;round front panel, 400mm,  horizontal connection, air supply, without regulating flap;MANDÍK;VVPM 400/K/V/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;0
VVPM 400/K/V/P/R;400;200;Anemostat;round front panel, 400mm,  horizontal connection, air supply, with regulating flap;MANDÍK;VVPM 400/K/V/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;0
VVPM 400/K/S/P;400;200;Anemostat;round front panel, 400mm,  vertical connection, air supply, without regulating flap;MANDÍK;VVPM 400/K/S/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;0
VVPM 400/K/S/P/R;400;200;Anemostat;round front panel, 400mm,  vertical connection, air supply, with regulating flap;MANDÍK;VVPM 400/K/S/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;0
VVPM 500/K/V/P;500;200;Anemostat;round front panel, 500mm,  horizontal connection, air supply, without regulating flap;MANDÍK;VVPM 500/K/V/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;0
VVPM 500/K/V/P/R;500;200;Anemostat;round front panel, 500mm,  horizontal connection, air supply, with regulating flap;MANDÍK;VVPM 500/K/V/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;0
VVPM 500/K/S/P;500;200;Anemostat;round front panel, 500mm,  vertical connection, air supply, without regulating flap;MANDÍK;VVPM 500/K/S/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;0
VVPM 500/K/S/P/R;500;200;Anemostat;round front panel, 500mm,  vertical connection, air supply, with regulating flap;MANDÍK;VVPM 500/K/S/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;0
VVPM 600/K/V/P;600;250;Anemostat;round front panel, 600mm,  horizontal connection, air supply, without regulating flap;MANDÍK;VVPM 600/K/V/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;0
VVPM 600/K/V/P/R;600;250;Anemostat;round front panel, 600mm,  horizontal connection, air supply, with regulating flap;MANDÍK;VVPM 600/K/V/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;0
VVPM 600/K/S/P;600;250;Anemostat;round front panel, 600mm,  vertical connection, air supply, without regulating flap;MANDÍK;VVPM 600/K/S/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;0
VVPM 600/K/S/P/R;600;250;Anemostat;round front panel, 600mm,  vertical connection, air supply, with regulating flap;MANDÍK;VVPM 600/K/S/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;0
VVPM 625/K/V/P;625;250;Anemostat;round front panel, 625mm,  horizontal connection, air supply, without regulating flap;MANDÍK;VVPM 625/K/V/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;0
VVPM 625/K/V/P/R;625;250;Anemostat;round front panel, 625mm,  horizontal connection, air supply, with regulating flap;MANDÍK;VVPM 625/K/V/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;0
VVPM 625/K/S/P;625;250;Anemostat;round front panel, 625mm,  vertical connection, air supply, without regulating flap;MANDÍK;VVPM 625/K/S/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;0
VVPM 625/K/S/P/R;625;250;Anemostat;round front panel, 625mm,  vertical connection, air supply, with regulating flap;MANDÍK;VVPM 625/K/S/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;0
VVPM 300/C fp supply;300;160;Anemostat;square front panel, 300mm, without regulating flap;MANDÍK;VVPM 300/C fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;1;1;1
VVPM 400/C fp supply;400;200;Anemostat;square front panel, 400mm, without regulating flap;MANDÍK;VVPM 400/C fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;1;1;1
VVPM 500/C fp supply;500;200;Anemostat;square front panel, 500mm, without regulating flap;MANDÍK;VVPM 500/C fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;1;1;1
VVPM 600/C fp supply;600;250;Anemostat;square front panel, 600mm, without regulating flap;MANDÍK;VVPM 600/C fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;1;1;1
VVPM 625/C fp supply;625;250;Anemostat;square front panel, 625mm, without regulating flap;MANDÍK;VVPM 625/C fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;1;1;1
VVPM 300/C/V/P;300;160;Anemostat;square front panel, 300mm,  horizontal connection, air supply, without regulating flap;MANDÍK;VVPM 300/C/V/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;1
VVPM 300/C/V/P/R;300;160;Anemostat;square front panel, 300mm,  horizontal connection, air supply, with regulating flap;MANDÍK;VVPM 300/C/V/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;1
VVPM 300/C/S/P;300;160;Anemostat;square front panel, 300mm,  vertical connection, air supply, without regulating flap;MANDÍK;VVPM 300/C/S/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;1
VVPM 300/C/S/P/R;300;160;Anemostat;square front panel, 300mm,  vertical connection, air supply, with regulating flap;MANDÍK;VVPM 300/C/S/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;1
VVPM 400/C/V/P;400;200;Anemostat;square front panel, 400mm,  horizontal connection, air supply, without regulating flap;MANDÍK;VVPM 400/C/V/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;1
VVPM 400/C/V/P/R;400;200;Anemostat;square front panel, 400mm,  horizontal connection, air supply, with regulating flap;MANDÍK;VVPM 400/C/V/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;1
VVPM 400/C/S/P;400;200;Anemostat;square front panel, 400mm,  vertical connection, air supply, without regulating flap;MANDÍK;VVPM 400/C/S/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;1
VVPM 400/C/S/P/R;400;200;Anemostat;square front panel, 400mm,  vertical connection, air supply, with regulating flap;MANDÍK;VVPM 400/C/S/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;1
VVPM 500/C/V/P;500;200;Anemostat;square front panel, 500mm,  horizontal connection, air supply, without regulating flap;MANDÍK;VVPM 500/C/V/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;1
VVPM 500/C/V/P/R;500;200;Anemostat;square front panel, 500mm,  horizontal connection, air supply, with regulating flap;MANDÍK;VVPM 500/C/V/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;1
VVPM 500/C/S/P;500;200;Anemostat;square front panel, 500mm,  vertical connection, air supply, without regulating flap;MANDÍK;VVPM 500/C/S/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;1
VVPM 500/C/S/P/R;500;200;Anemostat;square front panel, 500mm,  vertical connection, air supply, with regulating flap;MANDÍK;VVPM 500/C/S/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;1
VVPM 600/C/V/P;600;250;Anemostat;square front panel, 600mm,  horizontal connection, air supply, without regulating flap;MANDÍK;VVPM 600/C/V/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;1
VVPM 600/C/V/P/R;600;250;Anemostat;square front panel, 600mm,  horizontal connection, air supply, with regulating flap;MANDÍK;VVPM 600/C/V/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;1
VVPM 600/C/S/P;600;250;Anemostat;square front panel, 600mm,  vertical connection, air supply, without regulating flap;MANDÍK;VVPM 600/C/S/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;1
VVPM 600/C/S/P/R;600;250;Anemostat;square front panel, 600mm,  vertical connection, air supply, with regulating flap;MANDÍK;VVPM 600/C/S/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;1
VVPM 625/C/V/P;625;250;Anemostat;square front panel, 625mm,  horizontal connection, air supply, without regulating flap;MANDÍK;VVPM 625/C/V/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;1
VVPM 625/C/V/P/R;625;250;Anemostat;square front panel, 625mm,  horizontal connection, air supply, with regulating flap;MANDÍK;VVPM 625/C/V/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;0;1
VVPM 625/C/S/P;625;250;Anemostat;square front panel, 625mm,  vertical connection, air supply, without regulating flap;MANDÍK;VVPM 625/C/S/P;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;1
VVPM 625/C/S/P/R;625;250;Anemostat;square front panel, 625mm,  vertical connection, air supply, with regulating flap;MANDÍK;VVPM 625/C/S/P/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;0;1;1
VVPM 300/K fp supply;300;160;Anemostat;round front panel, 300mm, without regulating flap;MANDÍK;VVPM 300/K fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;1;1;0
VVPM 400/K fp supply;400;200;Anemostat;round front panel, 400mm, without regulating flap;MANDÍK;VVPM 400/K fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;1;1;0
VVPM 500/K fp supply;500;200;Anemostat;round front panel, 500mm, without regulating flap;MANDÍK;VVPM 500/K fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;1;1;0
VVPM 600/K fp supply;600;250;Anemostat;round front panel, 600mm, without regulating flap;MANDÍK;VVPM 600/K fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;1;1;0
VVPM 625/K fp supply;625;250;Anemostat;round front panel, 625mm, without regulating flap;MANDÍK;VVPM 625/K fp supply;https://www.mandik.cz/product-line/distribution-elements/anemostats/vvpm;1;1;0
