;Nominal dimension##LENGTH##MILLIMETERS;Description##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;Model##OTHER##;URL##OTHER##;Front panel##OTHER##;Upper connection##OTHER##;Side connection##OTHER##
VASM 315 V .01;315;Anemostat;horizontal connection, 315, manual, without regulating flap;MANDÍK;VASM 315 V .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 V .45;315;Anemostat;horizontal connection, 315, actuator controlled 230V, position regulation without signalling, without regulating flap;MANDÍK;VASM 315 V .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 V .46;315;Anemostat;horizontal connection, 315, actuator controlled 230V, position regulation with signalling, without regulating flap;MANDÍK;VASM 315 V .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 V .55;315;Anemostat;horizontal connection, 315, actuator controlled 24V, position regulation without signalling, without regulating flap;MANDÍK;VASM 315 V .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 V .56;315;Anemostat;horizontal connection, 315, actuator controlled 24V, position regulation with signalling, without regulating flap;MANDÍK;VASM 315 V .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 V .57;315;Anemostat;horizontal connection, 315, actuator controlled 24V SR, with smooth regulation, without regulating flap;MANDÍK;VASM 315 V .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 S .01;315;Anemostat;vertical connection, 315, manual, without regulating flap;MANDÍK;VASM 315 S .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 315 S .45;315;Anemostat;vertical connection, 315, actuator controlled 230V, position regulation without signalling, without regulating flap;MANDÍK;VASM 315 S .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 315 S .46;315;Anemostat;vertical connection, 315, actuator controlled 230V, position regulation with signalling, without regulating flap;MANDÍK;VASM 315 S .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 315 S .55;315;Anemostat;vertical connection, 315, actuator controlled 24V, position regulation without signalling, without regulating flap;MANDÍK;VASM 315 S .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 315 S .56;315;Anemostat;vertical connection, 315, actuator controlled 24V, position regulation with signalling, without regulating flap;MANDÍK;VASM 315 S .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 315 S .57;315;Anemostat;vertical connection, 315, actuator controlled 24V SR, with smooth regulation, without regulating flap;MANDÍK;VASM 315 S .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 V .01;400;Anemostat;horizontal connection, 400, manual, without regulating flap;MANDÍK;VASM 400 V .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 V .45;400;Anemostat;horizontal connection, 400, actuator controlled 230V, position regulation without signalling, without regulating flap;MANDÍK;VASM 400 V .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 V .46;400;Anemostat;horizontal connection, 400, actuator controlled 230V, position regulation with signalling, without regulating flap;MANDÍK;VASM 400 V .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 V .55;400;Anemostat;horizontal connection, 400, actuator controlled 24V, position regulation without signalling, without regulating flap;MANDÍK;VASM 400 V .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 V .56;400;Anemostat;horizontal connection, 400, actuator controlled 24V, position regulation with signalling, without regulating flap;MANDÍK;VASM 400 V .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 V .57;400;Anemostat;horizontal connection, 400, actuator controlled 24V SR, with smooth regulation, without regulating flap;MANDÍK;VASM 400 V .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 S .01;400;Anemostat;vertical connection, 400, manual, without regulating flap;MANDÍK;VASM 400 S .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 S .45;400;Anemostat;vertical connection, 400, actuator controlled 230V, position regulation without signalling, without regulating flap;MANDÍK;VASM 400 S .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 S .46;400;Anemostat;vertical connection, 400, actuator controlled 230V, position regulation with signalling, without regulating flap;MANDÍK;VASM 400 S .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 S .55;400;Anemostat;vertical connection, 400, actuator controlled 24V, position regulation without signalling, without regulating flap;MANDÍK;VASM 400 S .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 S .56;400;Anemostat;vertical connection, 400, actuator controlled 24V, position regulation with signalling, without regulating flap;MANDÍK;VASM 400 S .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 S .57;400;Anemostat;vertical connection, 400, actuator controlled 24V SR, with smooth regulation, without regulating flap;MANDÍK;VASM 400 S .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 V .01;630;Anemostat;horizontal connection, 630, manual, without regulating flap;MANDÍK;VASM 630 V .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 V .45;630;Anemostat;horizontal connection, 630, actuator controlled 230V, position regulation without signalling, without regulating flap;MANDÍK;VASM 630 V .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 V .46;630;Anemostat;horizontal connection, 630, actuator controlled 230V, position regulation with signalling, without regulating flap;MANDÍK;VASM 630 V .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 V .55;630;Anemostat;horizontal connection, 630, actuator controlled 24V, position regulation without signalling, without regulating flap;MANDÍK;VASM 630 V .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 V .56;630;Anemostat;horizontal connection, 630, actuator controlled 24V, position regulation with signalling, without regulating flap;MANDÍK;VASM 630 V .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 V .57;630;Anemostat;horizontal connection, 630, actuator controlled 24V SR, with smooth regulation, without regulating flap;MANDÍK;VASM 630 V .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 S .01;630;Anemostat;vertical connection, 630, manual, without regulating flap;MANDÍK;VASM 630 S .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 S .45;630;Anemostat;vertical connection, 630, actuator controlled 230V, position regulation without signalling, without regulating flap;MANDÍK;VASM 630 S .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 S .46;630;Anemostat;vertical connection, 630, actuator controlled 230V, position regulation with signalling, without regulating flap;MANDÍK;VASM 630 S .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 S .55;630;Anemostat;vertical connection, 630, actuator controlled 24V, position regulation without signalling, without regulating flap;MANDÍK;VASM 630 S .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 S .56;630;Anemostat;vertical connection, 630, actuator controlled 24V, position regulation with signalling, without regulating flap;MANDÍK;VASM 630 S .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 S .57;630;Anemostat;vertical connection, 630, actuator controlled 24V SR, with smooth regulation, without regulating flap;MANDÍK;VASM 630 S .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 315 fp supply .01;315;Anemostat;fp, 315, manual;MANDÍK;VASM 315 fp supply .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 315 fp supply .45;315;Anemostat;fp, 315, actuator controlled 230V, position regulation without signalling;MANDÍK;VASM 315 fp supply .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 315 fp supply .46;315;Anemostat;fp, 315, actuator controlled 230V, position regulation with signalling;MANDÍK;VASM 315 fp supply .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 315 fp supply .55;315;Anemostat;fp, 315, actuator controlled 24V, position regulation without signalling;MANDÍK;VASM 315 fp supply .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 315 fp supply .56;315;Anemostat;fp, 315, actuator controlled 24V, position regulation with signalling;MANDÍK;VASM 315 fp supply .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 315 fp supply .57;315;Anemostat;fp, 315, actuator controlled 24V SR, with smooth regulation;MANDÍK;VASM 315 fp supply .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 400 fp supply .01;400;Anemostat;fp, 400, manual;MANDÍK;VASM 400 fp supply .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 400 fp supply .45;400;Anemostat;fp, 400, actuator controlled 230V, position regulation without signalling;MANDÍK;VASM 400 fp supply .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 400 fp supply .46;400;Anemostat;fp, 400, actuator controlled 230V, position regulation with signalling;MANDÍK;VASM 400 fp supply .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 400 fp supply .55;400;Anemostat;fp, 400, actuator controlled 24V, position regulation without signalling;MANDÍK;VASM 400 fp supply .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 400 fp supply .56;400;Anemostat;fp, 400, actuator controlled 24V, position regulation with signalling;MANDÍK;VASM 400 fp supply .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 400 fp supply .57;400;Anemostat;fp, 400, actuator controlled 24V SR, with smooth regulation;MANDÍK;VASM 400 fp supply .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 630 fp supply .01;630;Anemostat;fp, 630, manual;MANDÍK;VASM 630 fp supply .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 630 fp supply .45;630;Anemostat;fp, 630, actuator controlled 230V, position regulation without signalling;MANDÍK;VASM 630 fp supply .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 630 fp supply .46;630;Anemostat;fp, 630, actuator controlled 230V, position regulation with signalling;MANDÍK;VASM 630 fp supply .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 630 fp supply .55;630;Anemostat;fp, 630, actuator controlled 24V, position regulation without signalling;MANDÍK;VASM 630 fp supply .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 630 fp supply .56;630;Anemostat;fp, 630, actuator controlled 24V, position regulation with signalling;MANDÍK;VASM 630 fp supply .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 630 fp supply .57;630;Anemostat;fp, 630, actuator controlled 24V SR, with smooth regulation;MANDÍK;VASM 630 fp supply .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;1;1;0
VASM 315 V/R .01;315;Anemostat;horizontal connection, 315, manual, with regulating flap;MANDÍK;VASM 315 V/R .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 V/R .45;315;Anemostat;horizontal connection, 315, actuator controlled 230V, position regulation without signalling, with regulating flap;MANDÍK;VASM 315 V/R .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 V/R .46;315;Anemostat;horizontal connection, 315, actuator controlled 230V, position regulation with signalling, with regulating flap;MANDÍK;VASM 315 V/R .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 V/R .55;315;Anemostat;horizontal connection, 315, actuator controlled 24V, position regulation without signalling, with regulating flap;MANDÍK;VASM 315 V/R .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 V/R .56;315;Anemostat;horizontal connection, 315, actuator controlled 24V, position regulation with signalling, with regulating flap;MANDÍK;VASM 315 V/R .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 V/R .57;315;Anemostat;horizontal connection, 315, actuator controlled 24V SR, with smooth regulation, with regulating flap;MANDÍK;VASM 315 V/R .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 315 S/R .01;315;Anemostat;vertical connection, 315, manual, with regulating flap;MANDÍK;VASM 315 S/R .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 315 S/R .45;315;Anemostat;vertical connection, 315, actuator controlled 230V, position regulation without signalling, with regulating flap;MANDÍK;VASM 315 S/R .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 315 S/R .46;315;Anemostat;vertical connection, 315, actuator controlled 230V, position regulation with signalling, with regulating flap;MANDÍK;VASM 315 S/R .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 315 S/R .55;315;Anemostat;vertical connection, 315, actuator controlled 24V, position regulation without signalling, with regulating flap;MANDÍK;VASM 315 S/R .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 315 S/R .56;315;Anemostat;vertical connection, 315, actuator controlled 24V, position regulation with signalling, with regulating flap;MANDÍK;VASM 315 S/R .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 315 S/R .57;315;Anemostat;vertical connection, 315, actuator controlled 24V SR, with smooth regulation, with regulating flap;MANDÍK;VASM 315 S/R .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 V/R .01;400;Anemostat;horizontal connection, 400, manual, with regulating flap;MANDÍK;VASM 400 V/R .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 V/R .45;400;Anemostat;horizontal connection, 400, actuator controlled 230V, position regulation without signalling, with regulating flap;MANDÍK;VASM 400 V/R .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 V/R .46;400;Anemostat;horizontal connection, 400, actuator controlled 230V, position regulation with signalling, with regulating flap;MANDÍK;VASM 400 V/R .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 V/R .55;400;Anemostat;horizontal connection, 400, actuator controlled 24V, position regulation without signalling, with regulating flap;MANDÍK;VASM 400 V/R .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 V/R .56;400;Anemostat;horizontal connection, 400, actuator controlled 24V, position regulation with signalling, with regulating flap;MANDÍK;VASM 400 V/R .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 V/R .57;400;Anemostat;horizontal connection, 400, actuator controlled 24V SR, with smooth regulation, with regulating flap;MANDÍK;VASM 400 V/R .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 400 S/R .01;400;Anemostat;vertical connection, 400, manual, with regulating flap;MANDÍK;VASM 400 S/R .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 S/R .45;400;Anemostat;vertical connection, 400, actuator controlled 230V, position regulation without signalling, with regulating flap;MANDÍK;VASM 400 S/R .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 S/R .46;400;Anemostat;vertical connection, 400, actuator controlled 230V, position regulation with signalling, with regulating flap;MANDÍK;VASM 400 S/R .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 S/R .55;400;Anemostat;vertical connection, 400, actuator controlled 24V, position regulation without signalling, with regulating flap;MANDÍK;VASM 400 S/R .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 S/R .56;400;Anemostat;vertical connection, 400, actuator controlled 24V, position regulation with signalling, with regulating flap;MANDÍK;VASM 400 S/R .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 400 S/R .57;400;Anemostat;vertical connection, 400, actuator controlled 24V SR, with smooth regulation, with regulating flap;MANDÍK;VASM 400 S/R .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 V/R .01;630;Anemostat;horizontal connection, 630, manual, with regulating flap;MANDÍK;VASM 630 V/R .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 V/R .45;630;Anemostat;horizontal connection, 630, actuator controlled 230V, position regulation without signalling, with regulating flap;MANDÍK;VASM 630 V/R .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 V/R .46;630;Anemostat;horizontal connection, 630, actuator controlled 230V, position regulation with signalling, with regulating flap;MANDÍK;VASM 630 V/R .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 V/R .55;630;Anemostat;horizontal connection, 630, actuator controlled 24V, position regulation without signalling, with regulating flap;MANDÍK;VASM 630 V/R .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 V/R .56;630;Anemostat;horizontal connection, 630, actuator controlled 24V, position regulation with signalling, with regulating flap;MANDÍK;VASM 630 V/R .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 V/R .57;630;Anemostat;horizontal connection, 630, actuator controlled 24V SR, with smooth regulation, with regulating flap;MANDÍK;VASM 630 V/R .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;0;1
VASM 630 S/R .01;630;Anemostat;vertical connection, 630, manual, with regulating flap;MANDÍK;VASM 630 S/R .01;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 S/R .45;630;Anemostat;vertical connection, 630, actuator controlled 230V, position regulation without signalling, with regulating flap;MANDÍK;VASM 630 S/R .45;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 S/R .46;630;Anemostat;vertical connection, 630, actuator controlled 230V, position regulation with signalling, with regulating flap;MANDÍK;VASM 630 S/R .46;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 S/R .55;630;Anemostat;vertical connection, 630, actuator controlled 24V, position regulation without signalling, with regulating flap;MANDÍK;VASM 630 S/R .55;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 S/R .56;630;Anemostat;vertical connection, 630, actuator controlled 24V, position regulation with signalling, with regulating flap;MANDÍK;VASM 630 S/R .56;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
VASM 630 S/R .57;630;Anemostat;vertical connection, 630, actuator controlled 24V SR, with smooth regulation, with regulating flap;MANDÍK;VASM 630 S/R .57;https://www.mandik.cz/product-line/distribution-elements/anemostats/vasm;0;1;0
