;Nominal width##LENGTH##MILLIMETERS;Nominal height##LENGTH##MILLIMETERS;DIAMETER##LENGTH##MILLIMETERS;Design##OTHER##;Duct width##OTHER##;Description##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;Model##OTHER##;URL##OTHER##;One-row##OTHER##;Two-row##OTHER##
VNKM 1 225x75/150;225;75;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 225x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 225x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x75/150;325;75;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 325x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 325x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x75/150;425;75;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 425x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 425x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x75/150;525;75;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 525x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 525x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x75/150;625;75;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 625x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 625x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x75/150;725;75;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 725x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 725x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x75/150;825;75;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 825x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 825x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x75/150;1025;75;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 1025x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x75/150;1225;75;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 1225x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x85/150;225;85;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 225x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 225x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x85/150;325;85;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 325x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 325x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x85/150;425;85;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 425x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 425x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x85/150;525;85;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 525x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 525x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x85/150;625;85;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 625x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 625x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x85/150;725;85;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 725x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 725x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x85/150;825;85;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 825x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 825x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x85/150;1025;85;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 1025x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x85/150;1225;85;150;1;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 1 1225x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x125/300;225;125;300;1;300 - 900;Vent;for one-row round duct, nominal dimensions 225x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 1 225x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x125/300;325;125;300;1;300 - 900;Vent;for one-row round duct, nominal dimensions 325x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 1 325x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x125/300;425;125;300;1;300 - 900;Vent;for one-row round duct, nominal dimensions 425x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 1 425x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x125/300;525;125;300;1;300 - 900;Vent;for one-row round duct, nominal dimensions 525x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 1 525x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x125/300;625;125;300;1;300 - 900;Vent;for one-row round duct, nominal dimensions 625x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 1 625x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x125/300;725;125;300;1;300 - 900;Vent;for one-row round duct, nominal dimensions 725x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 1 725x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x125/300;825;125;300;1;300 - 900;Vent;for one-row round duct, nominal dimensions 825x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 1 825x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x125/300;1025;125;300;1;300 - 900;Vent;for one-row round duct, nominal dimensions 1025x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 1 1025x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x125/300;1225;125;300;1;300 - 900;Vent;for one-row round duct, nominal dimensions 1225x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 1 1225x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x225/630;225;225;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 225x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x225/630;325;225;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 325x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x225/630;425;225;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 425x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x225/630;525;225;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 525x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x225/630;625;225;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 625x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x225/630;725;225;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 725x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x225/630;825;225;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 825x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x225/630;1025;225;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 1025x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x225/630;1225;225;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 1225x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x325/630;225;325;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 225x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x325/630;325;325;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 325x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x325/630;425;325;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 425x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x325/630;525;325;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 525x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x325/630;625;325;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 625x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x325/630;725;325;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 725x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x325/630;825;325;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 825x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x325/630;1025;325;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 1025x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x325/630;1225;325;630;1;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 1 1225x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x75/150/R1;225;75;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 225x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 225x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x75/150/R1;325;75;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 325x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 325x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x75/150/R1;425;75;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 425x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 425x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x75/150/R1;525;75;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 525x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 525x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x75/150/R1;625;75;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 625x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 625x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x75/150/R1;725;75;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 725x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 725x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x75/150/R1;825;75;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 825x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 825x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x75/150/R1;1025;75;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 1025x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x75/150/R1;1225;75;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 1225x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x85/150/R1;225;85;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 225x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 225x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x85/150/R1;325;85;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 325x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 325x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x85/150/R1;425;85;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 425x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 425x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x85/150/R1;525;85;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 525x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 525x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x85/150/R1;625;85;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 625x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 625x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x85/150/R1;725;85;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 725x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 725x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x85/150/R1;825;85;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 825x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 825x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x85/150/R1;1025;85;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 1025x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x85/150/R1;1225;85;150;1/R1;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 1 1225x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x125/300/R1;225;125;300;1/R1;300 - 900;Vent;for one-row round duct, nominal dimensions 225x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 1 225x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x125/300/R1;325;125;300;1/R1;300 - 900;Vent;for one-row round duct, nominal dimensions 325x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 1 325x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x125/300/R1;425;125;300;1/R1;300 - 900;Vent;for one-row round duct, nominal dimensions 425x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 1 425x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x125/300/R1;525;125;300;1/R1;300 - 900;Vent;for one-row round duct, nominal dimensions 525x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 1 525x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x125/300/R1;625;125;300;1/R1;300 - 900;Vent;for one-row round duct, nominal dimensions 625x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 1 625x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x125/300/R1;725;125;300;1/R1;300 - 900;Vent;for one-row round duct, nominal dimensions 725x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 1 725x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x125/300/R1;825;125;300;1/R1;300 - 900;Vent;for one-row round duct, nominal dimensions 825x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 1 825x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x125/300/R1;1025;125;300;1/R1;300 - 900;Vent;for one-row round duct, nominal dimensions 1025x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 1 1025x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x125/300/R1;1225;125;300;1/R1;300 - 900;Vent;for one-row round duct, nominal dimensions 1225x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 1 1225x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x225/630/R1;225;225;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 225x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x225/630/R1;325;225;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 325x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x225/630/R1;425;225;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 425x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x225/630/R1;525;225;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 525x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x225/630/R1;625;225;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 625x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x225/630/R1;725;225;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 725x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x225/630/R1;825;225;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 825x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x225/630/R1;1025;225;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 1025x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x225/630/R1;1225;225;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 1225x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x325/630/R1;225;325;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 225x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x325/630/R1;325;325;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 325x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x325/630/R1;425;325;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 425x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x325/630/R1;525;325;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 525x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x325/630/R1;625;325;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 625x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x325/630/R1;725;325;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 725x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x325/630/R1;825;325;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 825x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x325/630/R1;1025;325;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 1025x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x325/630/R1;1225;325;630;1/R1;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 1 1225x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x75/150/R2;225;75;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 225x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 225x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x75/150/R2;325;75;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 325x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 325x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x75/150/R2;425;75;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 425x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 425x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x75/150/R2;525;75;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 525x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 525x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x75/150/R2;625;75;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 625x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 625x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x75/150/R2;725;75;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 725x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 725x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x75/150/R2;825;75;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 825x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 825x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x75/150/R2;1025;75;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 1025x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x75/150/R2;1225;75;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 1225x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x85/150/R2;225;85;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 225x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 225x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x85/150/R2;325;85;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 325x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 325x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x85/150/R2;425;85;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 425x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 425x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x85/150/R2;525;85;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 525x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 525x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x85/150/R2;625;85;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 625x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 625x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x85/150/R2;725;85;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 725x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 725x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x85/150/R2;825;85;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 825x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 825x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x85/150/R2;1025;85;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 1025x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x85/150/R2;1225;85;150;1/R2;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 1 1225x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x125/300/R2;225;125;300;1/R2;300 - 900;Vent;for one-row round duct, nominal dimensions 225x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 1 225x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x125/300/R2;325;125;300;1/R2;300 - 900;Vent;for one-row round duct, nominal dimensions 325x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 1 325x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x125/300/R2;425;125;300;1/R2;300 - 900;Vent;for one-row round duct, nominal dimensions 425x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 1 425x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x125/300/R2;525;125;300;1/R2;300 - 900;Vent;for one-row round duct, nominal dimensions 525x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 1 525x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x125/300/R2;625;125;300;1/R2;300 - 900;Vent;for one-row round duct, nominal dimensions 625x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 1 625x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x125/300/R2;725;125;300;1/R2;300 - 900;Vent;for one-row round duct, nominal dimensions 725x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 1 725x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x125/300/R2;825;125;300;1/R2;300 - 900;Vent;for one-row round duct, nominal dimensions 825x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 1 825x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x125/300/R2;1025;125;300;1/R2;300 - 900;Vent;for one-row round duct, nominal dimensions 1025x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 1 1025x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x125/300/R2;1225;125;300;1/R2;300 - 900;Vent;for one-row round duct, nominal dimensions 1225x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 1 1225x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x225/630/R2;225;225;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 225x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x225/630/R2;325;225;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 325x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x225/630/R2;425;225;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 425x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x225/630/R2;525;225;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 525x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x225/630/R2;625;225;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 625x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x225/630/R2;725;225;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 725x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x225/630/R2;825;225;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 825x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x225/630/R2;1025;225;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 1025x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x225/630/R2;1225;225;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 1225x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x325/630/R2;225;325;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 225x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x325/630/R2;325;325;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 325x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x325/630/R2;425;325;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 425x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x325/630/R2;525;325;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 525x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x325/630/R2;625;325;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 625x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x325/630/R2;725;325;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 725x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x325/630/R2;825;325;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 825x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x325/630/R2;1025;325;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 1025x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x325/630/R2;1225;325;630;1/R2;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 1 1225x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x75/150/R3;225;75;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 225x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 225x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x75/150/R3;325;75;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 325x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 325x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x75/150/R3;425;75;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 425x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 425x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x75/150/R3;525;75;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 525x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 525x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x75/150/R3;625;75;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 625x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 625x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x75/150/R3;725;75;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 725x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 725x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x75/150/R3;825;75;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 825x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 825x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x75/150/R3;1025;75;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 1025x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x75/150/R3;1225;75;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 1225x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x85/150/R3;225;85;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 225x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 225x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x85/150/R3;325;85;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 325x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 325x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x85/150/R3;425;85;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 425x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 425x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x85/150/R3;525;85;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 525x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 525x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x85/150/R3;625;85;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 625x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 625x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x85/150/R3;725;85;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 725x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 725x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x85/150/R3;825;85;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 825x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 825x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x85/150/R3;1025;85;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 1025x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x85/150/R3;1225;85;150;1/R3;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 1 1225x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x125/300/R3;225;125;300;1/R3;300 - 900;Vent;for one-row round duct, nominal dimensions 225x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 1 225x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x125/300/R3;325;125;300;1/R3;300 - 900;Vent;for one-row round duct, nominal dimensions 325x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 1 325x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x125/300/R3;425;125;300;1/R3;300 - 900;Vent;for one-row round duct, nominal dimensions 425x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 1 425x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x125/300/R3;525;125;300;1/R3;300 - 900;Vent;for one-row round duct, nominal dimensions 525x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 1 525x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x125/300/R3;625;125;300;1/R3;300 - 900;Vent;for one-row round duct, nominal dimensions 625x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 1 625x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x125/300/R3;725;125;300;1/R3;300 - 900;Vent;for one-row round duct, nominal dimensions 725x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 1 725x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x125/300/R3;825;125;300;1/R3;300 - 900;Vent;for one-row round duct, nominal dimensions 825x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 1 825x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x125/300/R3;1025;125;300;1/R3;300 - 900;Vent;for one-row round duct, nominal dimensions 1025x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 1 1025x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x125/300/R3;1225;125;300;1/R3;300 - 900;Vent;for one-row round duct, nominal dimensions 1225x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 1 1225x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x225/630/R3;225;225;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 225x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x225/630/R3;325;225;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 325x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x225/630/R3;425;225;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 425x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x225/630/R3;525;225;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 525x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x225/630/R3;625;225;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 625x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x225/630/R3;725;225;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 725x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x225/630/R3;825;225;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 825x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x225/630/R3;1025;225;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 1025x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x225/630/R3;1225;225;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 1225x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x325/630/R3;225;325;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 225x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x325/630/R3;325;325;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 325x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x325/630/R3;425;325;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 425x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x325/630/R3;525;325;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 525x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x325/630/R3;625;325;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 625x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x325/630/R3;725;325;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 725x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x325/630/R3;825;325;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 825x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x325/630/R3;1025;325;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 1025x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x325/630/R3;1225;325;630;1/R3;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 1 1225x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x75/150/R5;225;75;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 225x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 225x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x75/150/R5;325;75;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 325x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 325x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x75/150/R5;425;75;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 425x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 425x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x75/150/R5;525;75;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 525x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 525x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x75/150/R5;625;75;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 625x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 625x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x75/150/R5;725;75;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 725x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 725x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x75/150/R5;825;75;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 825x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 825x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x75/150/R5;1025;75;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 1025x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x75/150/R5;1225;75;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 1225x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x85/150/R5;225;85;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 225x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 225x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x85/150/R5;325;85;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 325x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 325x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x85/150/R5;425;85;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 425x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 425x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x85/150/R5;525;85;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 525x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 525x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x85/150/R5;625;85;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 625x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 625x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x85/150/R5;725;85;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 725x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 725x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x85/150/R5;825;85;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 825x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 825x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x85/150/R5;1025;85;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 1025x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x85/150/R5;1225;85;150;1/R5;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 1 1225x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x125/300/R5;225;125;300;1/R5;300 - 900;Vent;for one-row round duct, nominal dimensions 225x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 1 225x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x125/300/R5;325;125;300;1/R5;300 - 900;Vent;for one-row round duct, nominal dimensions 325x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 1 325x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x125/300/R5;425;125;300;1/R5;300 - 900;Vent;for one-row round duct, nominal dimensions 425x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 1 425x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x125/300/R5;525;125;300;1/R5;300 - 900;Vent;for one-row round duct, nominal dimensions 525x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 1 525x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x125/300/R5;625;125;300;1/R5;300 - 900;Vent;for one-row round duct, nominal dimensions 625x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 1 625x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x125/300/R5;725;125;300;1/R5;300 - 900;Vent;for one-row round duct, nominal dimensions 725x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 1 725x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x125/300/R5;825;125;300;1/R5;300 - 900;Vent;for one-row round duct, nominal dimensions 825x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 1 825x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x125/300/R5;1025;125;300;1/R5;300 - 900;Vent;for one-row round duct, nominal dimensions 1025x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 1 1025x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x125/300/R5;1225;125;300;1/R5;300 - 900;Vent;for one-row round duct, nominal dimensions 1225x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 1 1225x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x225/630/R5;225;225;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 225x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x225/630/R5;325;225;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 325x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x225/630/R5;425;225;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 425x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x225/630/R5;525;225;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 525x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x225/630/R5;625;225;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 625x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x225/630/R5;725;225;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 725x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x225/630/R5;825;225;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 825x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x225/630/R5;1025;225;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 1025x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x225/630/R5;1225;225;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 1225x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x325/630/R5;225;325;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 225x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x325/630/R5;325;325;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 325x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x325/630/R5;425;325;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 425x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x325/630/R5;525;325;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 525x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x325/630/R5;625;325;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 625x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x325/630/R5;725;325;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 725x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x325/630/R5;825;325;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 825x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x325/630/R5;1025;325;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 1025x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x325/630/R5;1225;325;630;1/R5;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 1 1225x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x75/150/R6;225;75;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 225x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 225x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x75/150/R6;325;75;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 325x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 325x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x75/150/R6;425;75;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 425x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 425x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x75/150/R6;525;75;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 525x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 525x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x75/150/R6;625;75;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 625x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 625x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x75/150/R6;725;75;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 725x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 725x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x75/150/R6;825;75;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 825x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 825x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x75/150/R6;1025;75;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 1025x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x75/150/R6;1225;75;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 1225x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x85/150/R6;225;85;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 225x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 225x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x85/150/R6;325;85;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 325x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 325x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x85/150/R6;425;85;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 425x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 425x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x85/150/R6;525;85;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 525x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 525x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x85/150/R6;625;85;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 625x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 625x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x85/150/R6;725;85;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 725x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 725x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x85/150/R6;825;85;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 825x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 825x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x85/150/R6;1025;85;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 1025x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 1025x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x85/150/R6;1225;85;150;1/R6;150 - 400;Vent;for one-row round duct, nominal dimensions 1225x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 1 1225x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x125/300/R6;225;125;300;1/R6;300 - 900;Vent;for one-row round duct, nominal dimensions 225x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 1 225x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x125/300/R6;325;125;300;1/R6;300 - 900;Vent;for one-row round duct, nominal dimensions 325x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 1 325x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x125/300/R6;425;125;300;1/R6;300 - 900;Vent;for one-row round duct, nominal dimensions 425x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 1 425x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x125/300/R6;525;125;300;1/R6;300 - 900;Vent;for one-row round duct, nominal dimensions 525x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 1 525x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x125/300/R6;625;125;300;1/R6;300 - 900;Vent;for one-row round duct, nominal dimensions 625x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 1 625x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x125/300/R6;725;125;300;1/R6;300 - 900;Vent;for one-row round duct, nominal dimensions 725x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 1 725x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x125/300/R6;825;125;300;1/R6;300 - 900;Vent;for one-row round duct, nominal dimensions 825x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 1 825x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x125/300/R6;1025;125;300;1/R6;300 - 900;Vent;for one-row round duct, nominal dimensions 1025x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 1 1025x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x125/300/R6;1225;125;300;1/R6;300 - 900;Vent;for one-row round duct, nominal dimensions 1225x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 1 1225x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x225/630/R6;225;225;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 225x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x225/630/R6;325;225;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 325x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x225/630/R6;425;225;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 425x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x225/630/R6;525;225;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 525x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x225/630/R6;625;225;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 625x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x225/630/R6;725;225;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 725x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x225/630/R6;825;225;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 825x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x225/630/R6;1025;225;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 1025x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x225/630/R6;1225;225;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 1225x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 225x325/630/R6;225;325;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 225x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 225x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 325x325/630/R6;325;325;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 325x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 325x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 425x325/630/R6;425;325;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 425x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 425x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 525x325/630/R6;525;325;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 525x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 525x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 625x325/630/R6;625;325;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 625x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 625x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 725x325/630/R6;725;325;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 725x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 725x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 825x325/630/R6;825;325;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 825x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 825x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1025x325/630/R6;1025;325;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 1025x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 1 1225x325/630/R6;1225;325;630;1/R6;630 - 2400;Vent;for one-row round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 1 1225x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;1;0
VNKM 2 225x75/150;225;75;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 225x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x75/150;325;75;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 325x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x75/150;425;75;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 425x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x75/150;525;75;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 525x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x75/150;625;75;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 625x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x75/150;725;75;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 725x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x75/150;825;75;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 825x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x75/150;1025;75;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 1025x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x75/150;1225;75;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x75, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 1225x75/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x85/150;225;85;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 225x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x85/150;325;85;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 325x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x85/150;425;85;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 425x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x85/150;525;85;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 525x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x85/150;625;85;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 625x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x85/150;725;85;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 725x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x85/150;825;85;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 825x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x85/150;1025;85;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 1025x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x85/150;1225;85;150;2;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x85, duct diameter 150 - 400, without regulation;MANDÍK;VNKM 2 1225x85/150;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x125/300;225;125;300;2;300 - 900;Vent;for two-rows round duct, nominal dimensions 225x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 2 225x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x125/300;325;125;300;2;300 - 900;Vent;for two-rows round duct, nominal dimensions 325x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 2 325x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x125/300;425;125;300;2;300 - 900;Vent;for two-rows round duct, nominal dimensions 425x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 2 425x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x125/300;525;125;300;2;300 - 900;Vent;for two-rows round duct, nominal dimensions 525x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 2 525x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x125/300;625;125;300;2;300 - 900;Vent;for two-rows round duct, nominal dimensions 625x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 2 625x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x125/300;725;125;300;2;300 - 900;Vent;for two-rows round duct, nominal dimensions 725x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 2 725x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x125/300;825;125;300;2;300 - 900;Vent;for two-rows round duct, nominal dimensions 825x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 2 825x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x125/300;1025;125;300;2;300 - 900;Vent;for two-rows round duct, nominal dimensions 1025x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 2 1025x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x125/300;1225;125;300;2;300 - 900;Vent;for two-rows round duct, nominal dimensions 1225x125, duct diameter 300 - 900, without regulation;MANDÍK;VNKM 2 1225x125/300;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x225/630;225;225;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 225x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x225/630;325;225;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 325x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x225/630;425;225;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 425x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x225/630;525;225;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 525x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x225/630;625;225;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 625x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x225/630;725;225;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 725x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x225/630;825;225;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 825x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x225/630;1025;225;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 1025x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x225/630;1225;225;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 1225x225/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x325/630;225;325;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 225x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x325/630;325;325;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 325x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x325/630;425;325;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 425x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x325/630;525;325;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 525x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x325/630;625;325;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 625x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x325/630;725;325;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 725x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x325/630;825;325;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 825x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x325/630;1025;325;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 1025x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x325/630;1225;325;630;2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, without regulation;MANDÍK;VNKM 2 1225x325/630;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x75/150/R1;225;75;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 225x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x75/150/R1;325;75;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 325x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x75/150/R1;425;75;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 425x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x75/150/R1;525;75;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 525x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x75/150/R1;625;75;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 625x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x75/150/R1;725;75;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 725x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x75/150/R1;825;75;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 825x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x75/150/R1;1025;75;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 1025x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x75/150/R1;1225;75;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x75, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 1225x75/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x85/150/R1;225;85;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 225x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x85/150/R1;325;85;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 325x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x85/150/R1;425;85;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 425x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x85/150/R1;525;85;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 525x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x85/150/R1;625;85;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 625x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x85/150/R1;725;85;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 725x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x85/150/R1;825;85;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 825x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x85/150/R1;1025;85;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 1025x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x85/150/R1;1225;85;150;2/R1;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x85, duct diameter 150 - 400, with regulation 1;MANDÍK;VNKM 2 1225x85/150/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x125/300/R1;225;125;300;2/R1;300 - 900;Vent;for two-rows round duct, nominal dimensions 225x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 2 225x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x125/300/R1;325;125;300;2/R1;300 - 900;Vent;for two-rows round duct, nominal dimensions 325x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 2 325x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x125/300/R1;425;125;300;2/R1;300 - 900;Vent;for two-rows round duct, nominal dimensions 425x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 2 425x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x125/300/R1;525;125;300;2/R1;300 - 900;Vent;for two-rows round duct, nominal dimensions 525x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 2 525x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x125/300/R1;625;125;300;2/R1;300 - 900;Vent;for two-rows round duct, nominal dimensions 625x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 2 625x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x125/300/R1;725;125;300;2/R1;300 - 900;Vent;for two-rows round duct, nominal dimensions 725x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 2 725x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x125/300/R1;825;125;300;2/R1;300 - 900;Vent;for two-rows round duct, nominal dimensions 825x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 2 825x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x125/300/R1;1025;125;300;2/R1;300 - 900;Vent;for two-rows round duct, nominal dimensions 1025x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 2 1025x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x125/300/R1;1225;125;300;2/R1;300 - 900;Vent;for two-rows round duct, nominal dimensions 1225x125, duct diameter 300 - 900, with regulation 1;MANDÍK;VNKM 2 1225x125/300/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x225/630/R1;225;225;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 225x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x225/630/R1;325;225;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 325x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x225/630/R1;425;225;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 425x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x225/630/R1;525;225;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 525x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x225/630/R1;625;225;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 625x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x225/630/R1;725;225;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 725x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x225/630/R1;825;225;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 825x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x225/630/R1;1025;225;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 1025x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x225/630/R1;1225;225;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 1225x225/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x325/630/R1;225;325;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 225x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x325/630/R1;325;325;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 325x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x325/630/R1;425;325;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 425x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x325/630/R1;525;325;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 525x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x325/630/R1;625;325;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 625x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x325/630/R1;725;325;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 725x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x325/630/R1;825;325;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 825x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x325/630/R1;1025;325;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 1025x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x325/630/R1;1225;325;630;2/R1;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, with regulation 1;MANDÍK;VNKM 2 1225x325/630/R1;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x75/150/R2;225;75;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 225x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x75/150/R2;325;75;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 325x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x75/150/R2;425;75;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 425x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x75/150/R2;525;75;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 525x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x75/150/R2;625;75;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 625x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x75/150/R2;725;75;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 725x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x75/150/R2;825;75;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 825x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x75/150/R2;1025;75;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 1025x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x75/150/R2;1225;75;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x75, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 1225x75/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x85/150/R2;225;85;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 225x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x85/150/R2;325;85;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 325x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x85/150/R2;425;85;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 425x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x85/150/R2;525;85;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 525x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x85/150/R2;625;85;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 625x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x85/150/R2;725;85;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 725x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x85/150/R2;825;85;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 825x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x85/150/R2;1025;85;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 1025x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x85/150/R2;1225;85;150;2/R2;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x85, duct diameter 150 - 400, with regulation 2;MANDÍK;VNKM 2 1225x85/150/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x125/300/R2;225;125;300;2/R2;300 - 900;Vent;for two-rows round duct, nominal dimensions 225x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 2 225x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x125/300/R2;325;125;300;2/R2;300 - 900;Vent;for two-rows round duct, nominal dimensions 325x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 2 325x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x125/300/R2;425;125;300;2/R2;300 - 900;Vent;for two-rows round duct, nominal dimensions 425x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 2 425x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x125/300/R2;525;125;300;2/R2;300 - 900;Vent;for two-rows round duct, nominal dimensions 525x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 2 525x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x125/300/R2;625;125;300;2/R2;300 - 900;Vent;for two-rows round duct, nominal dimensions 625x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 2 625x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x125/300/R2;725;125;300;2/R2;300 - 900;Vent;for two-rows round duct, nominal dimensions 725x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 2 725x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x125/300/R2;825;125;300;2/R2;300 - 900;Vent;for two-rows round duct, nominal dimensions 825x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 2 825x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x125/300/R2;1025;125;300;2/R2;300 - 900;Vent;for two-rows round duct, nominal dimensions 1025x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 2 1025x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x125/300/R2;1225;125;300;2/R2;300 - 900;Vent;for two-rows round duct, nominal dimensions 1225x125, duct diameter 300 - 900, with regulation 2;MANDÍK;VNKM 2 1225x125/300/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x225/630/R2;225;225;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 225x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x225/630/R2;325;225;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 325x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x225/630/R2;425;225;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 425x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x225/630/R2;525;225;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 525x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x225/630/R2;625;225;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 625x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x225/630/R2;725;225;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 725x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x225/630/R2;825;225;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 825x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x225/630/R2;1025;225;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 1025x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x225/630/R2;1225;225;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 1225x225/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x325/630/R2;225;325;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 225x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x325/630/R2;325;325;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 325x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x325/630/R2;425;325;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 425x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x325/630/R2;525;325;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 525x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x325/630/R2;625;325;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 625x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x325/630/R2;725;325;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 725x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x325/630/R2;825;325;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 825x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x325/630/R2;1025;325;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 1025x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x325/630/R2;1225;325;630;2/R2;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, with regulation 2;MANDÍK;VNKM 2 1225x325/630/R2;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x75/150/R3;225;75;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 225x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x75/150/R3;325;75;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 325x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x75/150/R3;425;75;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 425x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x75/150/R3;525;75;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 525x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x75/150/R3;625;75;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 625x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x75/150/R3;725;75;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 725x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x75/150/R3;825;75;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 825x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x75/150/R3;1025;75;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 1025x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x75/150/R3;1225;75;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x75, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 1225x75/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x85/150/R3;225;85;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 225x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x85/150/R3;325;85;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 325x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x85/150/R3;425;85;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 425x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x85/150/R3;525;85;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 525x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x85/150/R3;625;85;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 625x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x85/150/R3;725;85;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 725x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x85/150/R3;825;85;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 825x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x85/150/R3;1025;85;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 1025x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x85/150/R3;1225;85;150;2/R3;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x85, duct diameter 150 - 400, with regulation 3;MANDÍK;VNKM 2 1225x85/150/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x125/300/R3;225;125;300;2/R3;300 - 900;Vent;for two-rows round duct, nominal dimensions 225x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 2 225x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x125/300/R3;325;125;300;2/R3;300 - 900;Vent;for two-rows round duct, nominal dimensions 325x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 2 325x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x125/300/R3;425;125;300;2/R3;300 - 900;Vent;for two-rows round duct, nominal dimensions 425x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 2 425x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x125/300/R3;525;125;300;2/R3;300 - 900;Vent;for two-rows round duct, nominal dimensions 525x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 2 525x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x125/300/R3;625;125;300;2/R3;300 - 900;Vent;for two-rows round duct, nominal dimensions 625x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 2 625x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x125/300/R3;725;125;300;2/R3;300 - 900;Vent;for two-rows round duct, nominal dimensions 725x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 2 725x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x125/300/R3;825;125;300;2/R3;300 - 900;Vent;for two-rows round duct, nominal dimensions 825x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 2 825x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x125/300/R3;1025;125;300;2/R3;300 - 900;Vent;for two-rows round duct, nominal dimensions 1025x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 2 1025x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x125/300/R3;1225;125;300;2/R3;300 - 900;Vent;for two-rows round duct, nominal dimensions 1225x125, duct diameter 300 - 900, with regulation 3;MANDÍK;VNKM 2 1225x125/300/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x225/630/R3;225;225;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 225x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x225/630/R3;325;225;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 325x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x225/630/R3;425;225;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 425x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x225/630/R3;525;225;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 525x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x225/630/R3;625;225;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 625x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x225/630/R3;725;225;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 725x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x225/630/R3;825;225;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 825x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x225/630/R3;1025;225;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 1025x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x225/630/R3;1225;225;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 1225x225/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x325/630/R3;225;325;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 225x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x325/630/R3;325;325;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 325x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x325/630/R3;425;325;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 425x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x325/630/R3;525;325;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 525x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x325/630/R3;625;325;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 625x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x325/630/R3;725;325;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 725x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x325/630/R3;825;325;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 825x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x325/630/R3;1025;325;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 1025x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x325/630/R3;1225;325;630;2/R3;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, with regulation 3;MANDÍK;VNKM 2 1225x325/630/R3;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x75/150/R5;225;75;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 225x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x75/150/R5;325;75;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 325x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x75/150/R5;425;75;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 425x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x75/150/R5;525;75;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 525x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x75/150/R5;625;75;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 625x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x75/150/R5;725;75;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 725x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x75/150/R5;825;75;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 825x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x75/150/R5;1025;75;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 1025x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x75/150/R5;1225;75;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x75, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 1225x75/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x85/150/R5;225;85;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 225x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x85/150/R5;325;85;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 325x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x85/150/R5;425;85;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 425x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x85/150/R5;525;85;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 525x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x85/150/R5;625;85;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 625x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x85/150/R5;725;85;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 725x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x85/150/R5;825;85;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 825x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x85/150/R5;1025;85;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 1025x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x85/150/R5;1225;85;150;2/R5;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x85, duct diameter 150 - 400, with regulation 5;MANDÍK;VNKM 2 1225x85/150/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x125/300/R5;225;125;300;2/R5;300 - 900;Vent;for two-rows round duct, nominal dimensions 225x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 2 225x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x125/300/R5;325;125;300;2/R5;300 - 900;Vent;for two-rows round duct, nominal dimensions 325x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 2 325x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x125/300/R5;425;125;300;2/R5;300 - 900;Vent;for two-rows round duct, nominal dimensions 425x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 2 425x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x125/300/R5;525;125;300;2/R5;300 - 900;Vent;for two-rows round duct, nominal dimensions 525x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 2 525x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x125/300/R5;625;125;300;2/R5;300 - 900;Vent;for two-rows round duct, nominal dimensions 625x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 2 625x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x125/300/R5;725;125;300;2/R5;300 - 900;Vent;for two-rows round duct, nominal dimensions 725x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 2 725x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x125/300/R5;825;125;300;2/R5;300 - 900;Vent;for two-rows round duct, nominal dimensions 825x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 2 825x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x125/300/R5;1025;125;300;2/R5;300 - 900;Vent;for two-rows round duct, nominal dimensions 1025x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 2 1025x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x125/300/R5;1225;125;300;2/R5;300 - 900;Vent;for two-rows round duct, nominal dimensions 1225x125, duct diameter 300 - 900, with regulation 5;MANDÍK;VNKM 2 1225x125/300/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x225/630/R5;225;225;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 225x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x225/630/R5;325;225;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 325x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x225/630/R5;425;225;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 425x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x225/630/R5;525;225;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 525x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x225/630/R5;625;225;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 625x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x225/630/R5;725;225;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 725x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x225/630/R5;825;225;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 825x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x225/630/R5;1025;225;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 1025x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x225/630/R5;1225;225;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 1225x225/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x325/630/R5;225;325;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 225x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x325/630/R5;325;325;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 325x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x325/630/R5;425;325;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 425x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x325/630/R5;525;325;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 525x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x325/630/R5;625;325;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 625x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x325/630/R5;725;325;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 725x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x325/630/R5;825;325;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 825x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x325/630/R5;1025;325;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 1025x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x325/630/R5;1225;325;630;2/R5;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, with regulation 5;MANDÍK;VNKM 2 1225x325/630/R5;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x75/150/R6;225;75;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 225x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x75/150/R6;325;75;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 325x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x75/150/R6;425;75;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 425x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x75/150/R6;525;75;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 525x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x75/150/R6;625;75;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 625x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x75/150/R6;725;75;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 725x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x75/150/R6;825;75;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 825x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x75/150/R6;1025;75;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 1025x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x75/150/R6;1225;75;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x75, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 1225x75/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x85/150/R6;225;85;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 225x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 225x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x85/150/R6;325;85;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 325x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 325x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x85/150/R6;425;85;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 425x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 425x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x85/150/R6;525;85;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 525x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 525x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x85/150/R6;625;85;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 625x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 625x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x85/150/R6;725;85;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 725x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 725x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x85/150/R6;825;85;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 825x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 825x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x85/150/R6;1025;85;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 1025x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 1025x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x85/150/R6;1225;85;150;2/R6;150 - 400;Vent;for two-rows round duct, nominal dimensions 1225x85, duct diameter 150 - 400, with regulation 6;MANDÍK;VNKM 2 1225x85/150/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x125/300/R6;225;125;300;2/R6;300 - 900;Vent;for two-rows round duct, nominal dimensions 225x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 2 225x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x125/300/R6;325;125;300;2/R6;300 - 900;Vent;for two-rows round duct, nominal dimensions 325x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 2 325x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x125/300/R6;425;125;300;2/R6;300 - 900;Vent;for two-rows round duct, nominal dimensions 425x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 2 425x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x125/300/R6;525;125;300;2/R6;300 - 900;Vent;for two-rows round duct, nominal dimensions 525x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 2 525x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x125/300/R6;625;125;300;2/R6;300 - 900;Vent;for two-rows round duct, nominal dimensions 625x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 2 625x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x125/300/R6;725;125;300;2/R6;300 - 900;Vent;for two-rows round duct, nominal dimensions 725x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 2 725x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x125/300/R6;825;125;300;2/R6;300 - 900;Vent;for two-rows round duct, nominal dimensions 825x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 2 825x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x125/300/R6;1025;125;300;2/R6;300 - 900;Vent;for two-rows round duct, nominal dimensions 1025x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 2 1025x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x125/300/R6;1225;125;300;2/R6;300 - 900;Vent;for two-rows round duct, nominal dimensions 1225x125, duct diameter 300 - 900, with regulation 6;MANDÍK;VNKM 2 1225x125/300/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x225/630/R6;225;225;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 225x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x225/630/R6;325;225;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 325x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x225/630/R6;425;225;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 425x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x225/630/R6;525;225;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 525x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x225/630/R6;625;225;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 625x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x225/630/R6;725;225;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 725x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x225/630/R6;825;225;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 825x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x225/630/R6;1025;225;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 1025x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x225/630/R6;1225;225;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x225, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 1225x225/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 225x325/630/R6;225;325;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 225x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 225x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 325x325/630/R6;325;325;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 325x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 325x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 425x325/630/R6;425;325;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 425x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 425x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 525x325/630/R6;525;325;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 525x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 525x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 625x325/630/R6;625;325;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 625x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 625x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 725x325/630/R6;725;325;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 725x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 725x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 825x325/630/R6;825;325;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 825x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 825x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1025x325/630/R6;1025;325;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1025x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 1025x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
VNKM 2 1225x325/630/R6;1225;325;630;2/R6;630 - 2400;Vent;for two-rows round duct, nominal dimensions 1225x325, duct diameter 630 - 2400, with regulation 6;MANDÍK;VNKM 2 1225x325/630/R6;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/vnkm;0;1
