;DUCT_DIAMETER##HVAC_DUCT_SIZE##MILLIMETERS;DUCT_DIAMETER 2##HVAC_DUCT_SIZE##MILLIMETERS;Kv##OTHER##;Dv##OTHER##;zero##OTHER##;Vv##OTHER##;Sv##OTHER##;SxV##OTHER##;Rk##OTHER##;Description##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;Model##OTHER##;URL##OTHER##
VAPM-V 160 K/D/V/O/R;160;125;1;1;0;1;0;0;1;Whirling anemostat;circular front plate, front plate with diffuser, horizontal connection, air outlet, with regulation flap;Mandík;VAPM-V 160 K/D/V/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 200 K/D/V/O/R;200;160;1;1;0;1;0;0;1;Whirling anemostat;circular front plate, front plate with diffuser, horizontal connection, air outlet, with regulation flap;Mandík;VAPM-V 200 K/D/V/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 250 K/D/V/O/R;250;200;1;1;0;1;0;0;1;Whirling anemostat;circular front plate, front plate with diffuser, horizontal connection, air outlet, with regulation flap;Mandík;VAPM-V 250 K/D/V/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 315 K/D/V/O/R;315;250;1;1;0;1;0;0;1;Whirling anemostat;circular front plate, front plate with diffuser, horizontal connection, air outlet, with regulation flap;Mandík;VAPM-V 315 K/D/V/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 160 K/D/V/O;160;125;1;1;0;1;0;0;0;Whirling anemostat;circular front plate, front plate with diffuser, horizontal connection, air outlet, without regulation flap;Mandík;VAPM-V 160 K/D/V/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 200 K/D/V/O;200;160;1;1;0;1;0;0;0;Whirling anemostat;circular front plate, front plate with diffuser, horizontal connection, air outlet, without regulation flap;Mandík;VAPM-V 200 K/D/V/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 250 K/D/V/O;250;200;1;1;0;1;0;0;0;Whirling anemostat;circular front plate, front plate with diffuser, horizontal connection, air outlet, without regulation flap;Mandík;VAPM-V 250 K/D/V/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 315 K/D/V/O;315;250;1;1;0;1;0;0;0;Whirling anemostat;circular front plate, front plate with diffuser, horizontal connection, air outlet, without regulation flap;Mandík;VAPM-V 315 K/D/V/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 160 K/D/S/O/R;160;125;1;1;0;0;1;1;1;Whirling anemostat;circular front plate, front plate with diffuser, vertical connection, air outlet, with regulation flap;Mandík;VAPM-V 160 K/D/S/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 200 K/D/S/O/R;200;160;1;1;0;0;1;1;1;Whirling anemostat;circular front plate, front plate with diffuser, vertical connection, air outlet, with regulation flap;Mandík;VAPM-V 200 K/D/S/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 250 K/D/S/O/R;250;200;1;1;0;0;1;1;1;Whirling anemostat;circular front plate, front plate with diffuser, vertical connection, air outlet, with regulation flap;Mandík;VAPM-V 250 K/D/S/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 315 K/D/S/O/R;315;250;1;1;0;0;1;1;1;Whirling anemostat;circular front plate, front plate with diffuser, vertical connection, air outlet, with regulation flap;Mandík;VAPM-V 315 K/D/S/O/R;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 160 K/D/S/O;160;125;1;1;0;0;1;1;0;Whirling anemostat;circular front plate, front plate with diffuser, vertical connection, air outlet, without regulation flap;Mandík;VAPM-V 160 K/D/S/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 200 K/D/S/O;200;160;1;1;0;0;1;1;0;Whirling anemostat;circular front plate, front plate with diffuser, vertical connection, air outlet, without regulation flap;Mandík;VAPM-V 200 K/D/S/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 250 K/D/S/O;250;200;1;1;0;0;1;1;0;Whirling anemostat;circular front plate, front plate with diffuser, vertical connection, air outlet, without regulation flap;Mandík;VAPM-V 250 K/D/S/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 315 K/D/S/O;315;250;1;1;0;0;1;1;0;Whirling anemostat;circular front plate, front plate with diffuser, vertical connection, air outlet, without regulation flap;Mandík;VAPM-V 315 K/D/S/O;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 160 K/D;160;160;1;1;1;0;0;1;0;Whirling anemostat;separate circular front plate, front plate with diffuser;Mandík;VAPM-V 160 K/D;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 200 K/D;200;200;1;1;1;0;0;1;0;Whirling anemostat;separate circular front plate, front plate with diffuser;Mandík;VAPM-V 200 K/D;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 250 K/D;250;250;1;1;1;0;0;1;0;Whirling anemostat;separate circular front plate, front plate with diffuser;Mandík;VAPM-V 250 K/D;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
VAPM-V 315 K/D;315;315;1;1;1;0;0;1;0;Whirling anemostat;separate circular front plate, front plate with diffuser;Mandík;VAPM-V 315 K/D;https://www.mandik.cz/product-line/distribution-elements/anemostats/vapm
