;Nominal width##LENGTH##MILLIMETERS;Nominal height##LENGTH##MILLIMETERS;Slat spacing##OTHER##;Design##OTHER##;Description##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;Model##OTHER##;URL##OTHER##
SMM 12,5 200x50 UR/S;200;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x75 UR/S;200;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x100 UR/S;200;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x125 UR/S;200;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x150 UR/S;200;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x200 UR/S;200;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x225 UR/S;200;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x250 UR/S;200;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x300 UR/S;200;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x325 UR/S;200;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x350 UR/S;200;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x400 UR/S;200;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x425 UR/S;200;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x450 UR/S;200;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x500 UR/S;200;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x525 UR/S;200;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 200x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x50 UR/S;225;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x75 UR/S;225;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x100 UR/S;225;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x125 UR/S;225;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x150 UR/S;225;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x200 UR/S;225;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x225 UR/S;225;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x250 UR/S;225;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x300 UR/S;225;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x325 UR/S;225;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x350 UR/S;225;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x400 UR/S;225;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x425 UR/S;225;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x450 UR/S;225;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x500 UR/S;225;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x525 UR/S;225;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 225x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x50 UR/S;300;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x75 UR/S;300;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x100 UR/S;300;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x125 UR/S;300;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x150 UR/S;300;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x200 UR/S;300;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x225 UR/S;300;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x250 UR/S;300;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x300 UR/S;300;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x325 UR/S;300;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x350 UR/S;300;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x400 UR/S;300;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x425 UR/S;300;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x450 UR/S;300;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x500 UR/S;300;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x525 UR/S;300;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 300x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x50 UR/S;325;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x75 UR/S;325;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x100 UR/S;325;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x125 UR/S;325;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x150 UR/S;325;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x200 UR/S;325;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x225 UR/S;325;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x250 UR/S;325;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x300 UR/S;325;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x325 UR/S;325;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x350 UR/S;325;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x400 UR/S;325;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x425 UR/S;325;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x450 UR/S;325;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x500 UR/S;325;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x525 UR/S;325;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 325x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x50 UR/S;400;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x75 UR/S;400;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x100 UR/S;400;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x125 UR/S;400;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x150 UR/S;400;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x200 UR/S;400;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x225 UR/S;400;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x250 UR/S;400;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x300 UR/S;400;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x325 UR/S;400;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x350 UR/S;400;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x400 UR/S;400;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x425 UR/S;400;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x450 UR/S;400;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x500 UR/S;400;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x525 UR/S;400;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 400x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x50 UR/S;425;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x75 UR/S;425;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x100 UR/S;425;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x125 UR/S;425;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x150 UR/S;425;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x200 UR/S;425;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x225 UR/S;425;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x250 UR/S;425;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x300 UR/S;425;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x325 UR/S;425;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x350 UR/S;425;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x400 UR/S;425;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x425 UR/S;425;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x450 UR/S;425;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x500 UR/S;425;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x525 UR/S;425;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 425x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x50 UR/S;500;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x75 UR/S;500;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x100 UR/S;500;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x125 UR/S;500;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x150 UR/S;500;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x200 UR/S;500;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x225 UR/S;500;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x250 UR/S;500;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x300 UR/S;500;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x325 UR/S;500;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x350 UR/S;500;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x400 UR/S;500;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x425 UR/S;500;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x450 UR/S;500;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x500 UR/S;500;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x525 UR/S;500;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 500x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x50 UR/S;525;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x75 UR/S;525;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x100 UR/S;525;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x125 UR/S;525;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x150 UR/S;525;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x200 UR/S;525;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x225 UR/S;525;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x250 UR/S;525;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x300 UR/S;525;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x325 UR/S;525;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x350 UR/S;525;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x400 UR/S;525;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x425 UR/S;525;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x450 UR/S;525;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x500 UR/S;525;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x525 UR/S;525;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 525x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x50 UR/S;600;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x75 UR/S;600;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x100 UR/S;600;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x125 UR/S;600;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x150 UR/S;600;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x200 UR/S;600;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x225 UR/S;600;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x250 UR/S;600;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x300 UR/S;600;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x325 UR/S;600;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x350 UR/S;600;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x400 UR/S;600;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x425 UR/S;600;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x450 UR/S;600;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x500 UR/S;600;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x525 UR/S;600;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 600x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x50 UR/S;625;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x75 UR/S;625;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x100 UR/S;625;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x125 UR/S;625;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x150 UR/S;625;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x200 UR/S;625;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x225 UR/S;625;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x250 UR/S;625;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x300 UR/S;625;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x325 UR/S;625;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x350 UR/S;625;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x400 UR/S;625;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x425 UR/S;625;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x450 UR/S;625;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x500 UR/S;625;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x525 UR/S;625;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 625x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x50 UR/S;700;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x75 UR/S;700;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x100 UR/S;700;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x125 UR/S;700;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x150 UR/S;700;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x200 UR/S;700;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x225 UR/S;700;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x250 UR/S;700;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x300 UR/S;700;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x325 UR/S;700;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x350 UR/S;700;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x400 UR/S;700;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x425 UR/S;700;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x450 UR/S;700;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x500 UR/S;700;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x525 UR/S;700;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 700x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x50 UR/S;725;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x75 UR/S;725;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x100 UR/S;725;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x125 UR/S;725;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x150 UR/S;725;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x200 UR/S;725;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x225 UR/S;725;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x250 UR/S;725;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x300 UR/S;725;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x325 UR/S;725;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x350 UR/S;725;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x400 UR/S;725;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x425 UR/S;725;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x450 UR/S;725;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x500 UR/S;725;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x525 UR/S;725;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 725x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x50 UR/S;800;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x75 UR/S;800;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x100 UR/S;800;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x125 UR/S;800;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x150 UR/S;800;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x200 UR/S;800;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x225 UR/S;800;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x250 UR/S;800;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x300 UR/S;800;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x325 UR/S;800;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x350 UR/S;800;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x400 UR/S;800;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x425 UR/S;800;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x450 UR/S;800;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x500 UR/S;800;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x525 UR/S;800;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 800x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x50 UR/S;825;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x75 UR/S;825;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x100 UR/S;825;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x125 UR/S;825;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x150 UR/S;825;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x200 UR/S;825;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x225 UR/S;825;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x250 UR/S;825;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x300 UR/S;825;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x325 UR/S;825;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x350 UR/S;825;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x400 UR/S;825;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x425 UR/S;825;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x450 UR/S;825;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x500 UR/S;825;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x525 UR/S;825;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 825x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x50 UR/S;1000;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x75 UR/S;1000;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x100 UR/S;1000;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x125 UR/S;1000;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x150 UR/S;1000;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x200 UR/S;1000;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x225 UR/S;1000;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x250 UR/S;1000;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x300 UR/S;1000;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x325 UR/S;1000;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x350 UR/S;1000;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x400 UR/S;1000;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x425 UR/S;1000;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x450 UR/S;1000;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x500 UR/S;1000;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x525 UR/S;1000;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1000x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x50 UR/S;1025;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x75 UR/S;1025;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x100 UR/S;1025;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x125 UR/S;1025;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x150 UR/S;1025;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x200 UR/S;1025;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x225 UR/S;1025;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x250 UR/S;1025;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x300 UR/S;1025;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x325 UR/S;1025;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x350 UR/S;1025;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x400 UR/S;1025;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x425 UR/S;1025;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x450 UR/S;1025;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x500 UR/S;1025;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x525 UR/S;1025;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1025x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x50 UR/S;1225;50;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x75 UR/S;1225;75;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x100 UR/S;1225;100;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x125 UR/S;1225;125;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x150 UR/S;1225;150;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x200 UR/S;1225;200;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x225 UR/S;1225;225;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x250 UR/S;1225;250;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x300 UR/S;1225;300;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x325 UR/S;1225;325;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x350 UR/S;1225;350;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x400 UR/S;1225;400;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x425 UR/S;1225;425;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x450 UR/S;1225;450;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x500 UR/S;1225;500;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x525 UR/S;1225;525;12,5;UR;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 12,5 1225x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x50 UR/S;200;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x75 UR/S;200;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x100 UR/S;200;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x125 UR/S;200;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x150 UR/S;200;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x200 UR/S;200;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x225 UR/S;200;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x250 UR/S;200;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x300 UR/S;200;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x325 UR/S;200;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x350 UR/S;200;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x400 UR/S;200;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x425 UR/S;200;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x450 UR/S;200;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x500 UR/S;200;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x525 UR/S;200;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 200x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 200x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x50 UR/S;225;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x75 UR/S;225;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x100 UR/S;225;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x125 UR/S;225;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x150 UR/S;225;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x200 UR/S;225;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x225 UR/S;225;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x250 UR/S;225;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x300 UR/S;225;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x325 UR/S;225;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x350 UR/S;225;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x400 UR/S;225;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x425 UR/S;225;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x450 UR/S;225;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x500 UR/S;225;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x525 UR/S;225;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 225x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 225x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x50 UR/S;300;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x75 UR/S;300;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x100 UR/S;300;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x125 UR/S;300;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x150 UR/S;300;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x200 UR/S;300;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x225 UR/S;300;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x250 UR/S;300;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x300 UR/S;300;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x325 UR/S;300;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x350 UR/S;300;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x400 UR/S;300;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x425 UR/S;300;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x450 UR/S;300;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x500 UR/S;300;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x525 UR/S;300;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 300x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 300x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x50 UR/S;325;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x75 UR/S;325;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x100 UR/S;325;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x125 UR/S;325;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x150 UR/S;325;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x200 UR/S;325;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x225 UR/S;325;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x250 UR/S;325;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x300 UR/S;325;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x325 UR/S;325;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x350 UR/S;325;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x400 UR/S;325;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x425 UR/S;325;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x450 UR/S;325;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x500 UR/S;325;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x525 UR/S;325;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 325x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 325x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x50 UR/S;400;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x75 UR/S;400;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x100 UR/S;400;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x125 UR/S;400;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x150 UR/S;400;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x200 UR/S;400;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x225 UR/S;400;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x250 UR/S;400;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x300 UR/S;400;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x325 UR/S;400;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x350 UR/S;400;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x400 UR/S;400;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x425 UR/S;400;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x450 UR/S;400;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x500 UR/S;400;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x525 UR/S;400;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 400x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 400x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x50 UR/S;425;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x75 UR/S;425;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x100 UR/S;425;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x125 UR/S;425;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x150 UR/S;425;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x200 UR/S;425;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x225 UR/S;425;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x250 UR/S;425;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x300 UR/S;425;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x325 UR/S;425;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x350 UR/S;425;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x400 UR/S;425;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x425 UR/S;425;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x450 UR/S;425;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x500 UR/S;425;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x525 UR/S;425;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 425x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 425x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x50 UR/S;500;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x75 UR/S;500;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x100 UR/S;500;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x125 UR/S;500;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x150 UR/S;500;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x200 UR/S;500;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x225 UR/S;500;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x250 UR/S;500;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x300 UR/S;500;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x325 UR/S;500;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x350 UR/S;500;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x400 UR/S;500;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x425 UR/S;500;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x450 UR/S;500;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x500 UR/S;500;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x525 UR/S;500;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 500x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 500x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x50 UR/S;525;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x75 UR/S;525;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x100 UR/S;525;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x125 UR/S;525;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x150 UR/S;525;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x200 UR/S;525;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x225 UR/S;525;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x250 UR/S;525;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x300 UR/S;525;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x325 UR/S;525;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x350 UR/S;525;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x400 UR/S;525;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x425 UR/S;525;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x450 UR/S;525;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x500 UR/S;525;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x525 UR/S;525;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 525x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 525x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x50 UR/S;600;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x75 UR/S;600;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x100 UR/S;600;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x125 UR/S;600;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x150 UR/S;600;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x200 UR/S;600;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x225 UR/S;600;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x250 UR/S;600;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x300 UR/S;600;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x325 UR/S;600;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x350 UR/S;600;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x400 UR/S;600;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x425 UR/S;600;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x450 UR/S;600;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x500 UR/S;600;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x525 UR/S;600;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 600x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 600x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x50 UR/S;625;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x75 UR/S;625;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x100 UR/S;625;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x125 UR/S;625;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x150 UR/S;625;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x200 UR/S;625;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x225 UR/S;625;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x250 UR/S;625;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x300 UR/S;625;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x325 UR/S;625;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x350 UR/S;625;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x400 UR/S;625;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x425 UR/S;625;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x450 UR/S;625;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x500 UR/S;625;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x525 UR/S;625;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 625x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 625x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x50 UR/S;700;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x75 UR/S;700;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x100 UR/S;700;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x125 UR/S;700;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x150 UR/S;700;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x200 UR/S;700;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x225 UR/S;700;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x250 UR/S;700;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x300 UR/S;700;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x325 UR/S;700;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x350 UR/S;700;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x400 UR/S;700;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x425 UR/S;700;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x450 UR/S;700;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x500 UR/S;700;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x525 UR/S;700;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 700x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 700x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x50 UR/S;725;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x75 UR/S;725;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x100 UR/S;725;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x125 UR/S;725;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x150 UR/S;725;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x200 UR/S;725;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x225 UR/S;725;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x250 UR/S;725;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x300 UR/S;725;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x325 UR/S;725;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x350 UR/S;725;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x400 UR/S;725;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x425 UR/S;725;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x450 UR/S;725;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x500 UR/S;725;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x525 UR/S;725;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 725x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 725x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x50 UR/S;800;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x75 UR/S;800;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x100 UR/S;800;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x125 UR/S;800;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x150 UR/S;800;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x200 UR/S;800;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x225 UR/S;800;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x250 UR/S;800;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x300 UR/S;800;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x325 UR/S;800;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x350 UR/S;800;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x400 UR/S;800;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x425 UR/S;800;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x450 UR/S;800;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x500 UR/S;800;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x525 UR/S;800;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 800x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 800x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x50 UR/S;825;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x75 UR/S;825;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x100 UR/S;825;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x125 UR/S;825;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x150 UR/S;825;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x200 UR/S;825;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x225 UR/S;825;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x250 UR/S;825;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x300 UR/S;825;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x325 UR/S;825;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x350 UR/S;825;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x400 UR/S;825;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x425 UR/S;825;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x450 UR/S;825;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x500 UR/S;825;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x525 UR/S;825;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 825x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 825x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x50 UR/S;1000;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x75 UR/S;1000;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x100 UR/S;1000;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x125 UR/S;1000;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x150 UR/S;1000;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x200 UR/S;1000;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x225 UR/S;1000;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x250 UR/S;1000;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x300 UR/S;1000;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x325 UR/S;1000;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x350 UR/S;1000;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x400 UR/S;1000;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x425 UR/S;1000;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x450 UR/S;1000;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x500 UR/S;1000;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x525 UR/S;1000;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1000x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x50 UR/S;1025;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x75 UR/S;1025;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x100 UR/S;1025;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x125 UR/S;1025;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x150 UR/S;1025;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x200 UR/S;1025;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x225 UR/S;1025;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x250 UR/S;1025;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x300 UR/S;1025;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x325 UR/S;1025;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x350 UR/S;1025;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x400 UR/S;1025;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x425 UR/S;1025;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x450 UR/S;1025;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x500 UR/S;1025;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x525 UR/S;1025;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1025x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x50 UR/S;1225;50;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x50, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x50 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x75 UR/S;1225;75;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x75, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x75 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x100 UR/S;1225;100;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x100, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x100 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x125 UR/S;1225;125;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x125, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x125 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x150 UR/S;1225;150;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x150, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x150 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x200 UR/S;1225;200;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x200, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x200 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x225 UR/S;1225;225;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x225, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x225 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x250 UR/S;1225;250;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x250, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x250 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x300 UR/S;1225;300;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x300, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x300 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x325 UR/S;1225;325;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x325, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x325 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x350 UR/S;1225;350;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x350, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x350 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x400 UR/S;1225;400;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x400, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x400 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x425 UR/S;1225;425;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x425, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x425 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x450 UR/S;1225;450;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x450, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x450 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x500 UR/S;1225;500;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x500, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x500 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x525 UR/S;1225;525;20;UR;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x525, mounting frame without brackets, screw fastening;MANDÍK;SMM 20 1225x525 UR/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x50 UR1/S;200;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x75 UR1/S;200;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x100 UR1/S;200;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x125 UR1/S;200;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x150 UR1/S;200;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x200 UR1/S;200;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x225 UR1/S;200;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x250 UR1/S;200;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x300 UR1/S;200;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x325 UR1/S;200;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x350 UR1/S;200;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x400 UR1/S;200;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x425 UR1/S;200;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x450 UR1/S;200;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x500 UR1/S;200;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x525 UR1/S;200;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 200x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x50 UR1/S;225;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x75 UR1/S;225;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x100 UR1/S;225;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x125 UR1/S;225;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x150 UR1/S;225;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x200 UR1/S;225;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x225 UR1/S;225;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x250 UR1/S;225;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x300 UR1/S;225;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x325 UR1/S;225;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x350 UR1/S;225;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x400 UR1/S;225;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x425 UR1/S;225;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x450 UR1/S;225;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x500 UR1/S;225;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x525 UR1/S;225;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 225x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x50 UR1/S;300;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x75 UR1/S;300;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x100 UR1/S;300;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x125 UR1/S;300;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x150 UR1/S;300;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x200 UR1/S;300;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x225 UR1/S;300;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x250 UR1/S;300;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x300 UR1/S;300;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x325 UR1/S;300;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x350 UR1/S;300;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x400 UR1/S;300;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x425 UR1/S;300;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x450 UR1/S;300;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x500 UR1/S;300;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x525 UR1/S;300;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 300x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x50 UR1/S;325;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x75 UR1/S;325;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x100 UR1/S;325;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x125 UR1/S;325;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x150 UR1/S;325;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x200 UR1/S;325;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x225 UR1/S;325;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x250 UR1/S;325;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x300 UR1/S;325;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x325 UR1/S;325;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x350 UR1/S;325;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x400 UR1/S;325;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x425 UR1/S;325;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x450 UR1/S;325;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x500 UR1/S;325;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x525 UR1/S;325;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 325x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x50 UR1/S;400;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x75 UR1/S;400;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x100 UR1/S;400;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x125 UR1/S;400;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x150 UR1/S;400;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x200 UR1/S;400;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x225 UR1/S;400;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x250 UR1/S;400;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x300 UR1/S;400;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x325 UR1/S;400;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x350 UR1/S;400;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x400 UR1/S;400;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x425 UR1/S;400;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x450 UR1/S;400;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x500 UR1/S;400;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x525 UR1/S;400;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 400x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x50 UR1/S;425;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x75 UR1/S;425;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x100 UR1/S;425;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x125 UR1/S;425;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x150 UR1/S;425;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x200 UR1/S;425;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x225 UR1/S;425;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x250 UR1/S;425;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x300 UR1/S;425;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x325 UR1/S;425;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x350 UR1/S;425;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x400 UR1/S;425;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x425 UR1/S;425;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x450 UR1/S;425;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x500 UR1/S;425;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x525 UR1/S;425;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 425x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x50 UR1/S;500;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x75 UR1/S;500;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x100 UR1/S;500;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x125 UR1/S;500;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x150 UR1/S;500;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x200 UR1/S;500;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x225 UR1/S;500;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x250 UR1/S;500;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x300 UR1/S;500;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x325 UR1/S;500;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x350 UR1/S;500;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x400 UR1/S;500;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x425 UR1/S;500;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x450 UR1/S;500;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x500 UR1/S;500;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x525 UR1/S;500;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 500x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x50 UR1/S;525;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x75 UR1/S;525;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x100 UR1/S;525;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x125 UR1/S;525;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x150 UR1/S;525;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x200 UR1/S;525;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x225 UR1/S;525;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x250 UR1/S;525;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x300 UR1/S;525;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x325 UR1/S;525;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x350 UR1/S;525;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x400 UR1/S;525;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x425 UR1/S;525;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x450 UR1/S;525;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x500 UR1/S;525;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x525 UR1/S;525;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 525x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x50 UR1/S;600;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x75 UR1/S;600;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x100 UR1/S;600;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x125 UR1/S;600;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x150 UR1/S;600;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x200 UR1/S;600;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x225 UR1/S;600;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x250 UR1/S;600;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x300 UR1/S;600;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x325 UR1/S;600;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x350 UR1/S;600;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x400 UR1/S;600;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x425 UR1/S;600;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x450 UR1/S;600;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x500 UR1/S;600;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x525 UR1/S;600;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 600x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x50 UR1/S;625;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x75 UR1/S;625;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x100 UR1/S;625;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x125 UR1/S;625;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x150 UR1/S;625;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x200 UR1/S;625;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x225 UR1/S;625;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x250 UR1/S;625;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x300 UR1/S;625;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x325 UR1/S;625;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x350 UR1/S;625;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x400 UR1/S;625;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x425 UR1/S;625;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x450 UR1/S;625;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x500 UR1/S;625;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x525 UR1/S;625;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 625x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x50 UR1/S;700;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x75 UR1/S;700;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x100 UR1/S;700;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x125 UR1/S;700;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x150 UR1/S;700;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x200 UR1/S;700;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x225 UR1/S;700;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x250 UR1/S;700;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x300 UR1/S;700;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x325 UR1/S;700;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x350 UR1/S;700;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x400 UR1/S;700;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x425 UR1/S;700;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x450 UR1/S;700;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x500 UR1/S;700;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x525 UR1/S;700;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 700x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x50 UR1/S;725;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x75 UR1/S;725;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x100 UR1/S;725;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x125 UR1/S;725;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x150 UR1/S;725;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x200 UR1/S;725;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x225 UR1/S;725;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x250 UR1/S;725;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x300 UR1/S;725;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x325 UR1/S;725;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x350 UR1/S;725;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x400 UR1/S;725;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x425 UR1/S;725;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x450 UR1/S;725;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x500 UR1/S;725;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x525 UR1/S;725;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 725x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x50 UR1/S;800;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x75 UR1/S;800;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x100 UR1/S;800;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x125 UR1/S;800;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x150 UR1/S;800;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x200 UR1/S;800;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x225 UR1/S;800;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x250 UR1/S;800;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x300 UR1/S;800;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x325 UR1/S;800;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x350 UR1/S;800;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x400 UR1/S;800;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x425 UR1/S;800;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x450 UR1/S;800;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x500 UR1/S;800;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x525 UR1/S;800;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 800x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x50 UR1/S;825;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x75 UR1/S;825;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x100 UR1/S;825;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x125 UR1/S;825;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x150 UR1/S;825;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x200 UR1/S;825;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x225 UR1/S;825;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x250 UR1/S;825;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x300 UR1/S;825;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x325 UR1/S;825;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x350 UR1/S;825;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x400 UR1/S;825;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x425 UR1/S;825;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x450 UR1/S;825;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x500 UR1/S;825;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x525 UR1/S;825;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 825x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x50 UR1/S;1000;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x75 UR1/S;1000;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x100 UR1/S;1000;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x125 UR1/S;1000;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x150 UR1/S;1000;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x200 UR1/S;1000;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x225 UR1/S;1000;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x250 UR1/S;1000;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x300 UR1/S;1000;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x325 UR1/S;1000;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x350 UR1/S;1000;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x400 UR1/S;1000;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x425 UR1/S;1000;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x450 UR1/S;1000;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x500 UR1/S;1000;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x525 UR1/S;1000;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1000x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x50 UR1/S;1025;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x75 UR1/S;1025;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x100 UR1/S;1025;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x125 UR1/S;1025;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x150 UR1/S;1025;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x200 UR1/S;1025;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x225 UR1/S;1025;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x250 UR1/S;1025;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x300 UR1/S;1025;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x325 UR1/S;1025;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x350 UR1/S;1025;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x400 UR1/S;1025;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x425 UR1/S;1025;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x450 UR1/S;1025;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x500 UR1/S;1025;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x525 UR1/S;1025;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1025x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x50 UR1/S;1225;50;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x75 UR1/S;1225;75;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x100 UR1/S;1225;100;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x125 UR1/S;1225;125;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x150 UR1/S;1225;150;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x200 UR1/S;1225;200;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x225 UR1/S;1225;225;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x250 UR1/S;1225;250;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x300 UR1/S;1225;300;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x325 UR1/S;1225;325;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x350 UR1/S;1225;350;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x400 UR1/S;1225;400;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x425 UR1/S;1225;425;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x450 UR1/S;1225;450;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x500 UR1/S;1225;500;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x525 UR1/S;1225;525;12,5;UR1;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 12,5 1225x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x50 UR1/S;200;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x75 UR1/S;200;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x100 UR1/S;200;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x125 UR1/S;200;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x150 UR1/S;200;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x200 UR1/S;200;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x225 UR1/S;200;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x250 UR1/S;200;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x300 UR1/S;200;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x325 UR1/S;200;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x350 UR1/S;200;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x400 UR1/S;200;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x425 UR1/S;200;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x450 UR1/S;200;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x500 UR1/S;200;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x525 UR1/S;200;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 200x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 200x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x50 UR1/S;225;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x75 UR1/S;225;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x100 UR1/S;225;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x125 UR1/S;225;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x150 UR1/S;225;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x200 UR1/S;225;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x225 UR1/S;225;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x250 UR1/S;225;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x300 UR1/S;225;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x325 UR1/S;225;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x350 UR1/S;225;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x400 UR1/S;225;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x425 UR1/S;225;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x450 UR1/S;225;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x500 UR1/S;225;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x525 UR1/S;225;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 225x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 225x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x50 UR1/S;300;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x75 UR1/S;300;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x100 UR1/S;300;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x125 UR1/S;300;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x150 UR1/S;300;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x200 UR1/S;300;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x225 UR1/S;300;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x250 UR1/S;300;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x300 UR1/S;300;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x325 UR1/S;300;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x350 UR1/S;300;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x400 UR1/S;300;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x425 UR1/S;300;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x450 UR1/S;300;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x500 UR1/S;300;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x525 UR1/S;300;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 300x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 300x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x50 UR1/S;325;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x75 UR1/S;325;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x100 UR1/S;325;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x125 UR1/S;325;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x150 UR1/S;325;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x200 UR1/S;325;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x225 UR1/S;325;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x250 UR1/S;325;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x300 UR1/S;325;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x325 UR1/S;325;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x350 UR1/S;325;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x400 UR1/S;325;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x425 UR1/S;325;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x450 UR1/S;325;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x500 UR1/S;325;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x525 UR1/S;325;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 325x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 325x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x50 UR1/S;400;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x75 UR1/S;400;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x100 UR1/S;400;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x125 UR1/S;400;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x150 UR1/S;400;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x200 UR1/S;400;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x225 UR1/S;400;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x250 UR1/S;400;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x300 UR1/S;400;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x325 UR1/S;400;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x350 UR1/S;400;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x400 UR1/S;400;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x425 UR1/S;400;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x450 UR1/S;400;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x500 UR1/S;400;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x525 UR1/S;400;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 400x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 400x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x50 UR1/S;425;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x75 UR1/S;425;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x100 UR1/S;425;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x125 UR1/S;425;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x150 UR1/S;425;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x200 UR1/S;425;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x225 UR1/S;425;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x250 UR1/S;425;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x300 UR1/S;425;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x325 UR1/S;425;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x350 UR1/S;425;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x400 UR1/S;425;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x425 UR1/S;425;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x450 UR1/S;425;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x500 UR1/S;425;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x525 UR1/S;425;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 425x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 425x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x50 UR1/S;500;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x75 UR1/S;500;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x100 UR1/S;500;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x125 UR1/S;500;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x150 UR1/S;500;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x200 UR1/S;500;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x225 UR1/S;500;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x250 UR1/S;500;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x300 UR1/S;500;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x325 UR1/S;500;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x350 UR1/S;500;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x400 UR1/S;500;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x425 UR1/S;500;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x450 UR1/S;500;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x500 UR1/S;500;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x525 UR1/S;500;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 500x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 500x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x50 UR1/S;525;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x75 UR1/S;525;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x100 UR1/S;525;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x125 UR1/S;525;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x150 UR1/S;525;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x200 UR1/S;525;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x225 UR1/S;525;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x250 UR1/S;525;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x300 UR1/S;525;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x325 UR1/S;525;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x350 UR1/S;525;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x400 UR1/S;525;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x425 UR1/S;525;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x450 UR1/S;525;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x500 UR1/S;525;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x525 UR1/S;525;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 525x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 525x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x50 UR1/S;600;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x75 UR1/S;600;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x100 UR1/S;600;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x125 UR1/S;600;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x150 UR1/S;600;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x200 UR1/S;600;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x225 UR1/S;600;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x250 UR1/S;600;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x300 UR1/S;600;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x325 UR1/S;600;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x350 UR1/S;600;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x400 UR1/S;600;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x425 UR1/S;600;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x450 UR1/S;600;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x500 UR1/S;600;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x525 UR1/S;600;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 600x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 600x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x50 UR1/S;625;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x75 UR1/S;625;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x100 UR1/S;625;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x125 UR1/S;625;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x150 UR1/S;625;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x200 UR1/S;625;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x225 UR1/S;625;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x250 UR1/S;625;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x300 UR1/S;625;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x325 UR1/S;625;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x350 UR1/S;625;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x400 UR1/S;625;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x425 UR1/S;625;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x450 UR1/S;625;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x500 UR1/S;625;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x525 UR1/S;625;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 625x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 625x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x50 UR1/S;700;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x75 UR1/S;700;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x100 UR1/S;700;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x125 UR1/S;700;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x150 UR1/S;700;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x200 UR1/S;700;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x225 UR1/S;700;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x250 UR1/S;700;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x300 UR1/S;700;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x325 UR1/S;700;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x350 UR1/S;700;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x400 UR1/S;700;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x425 UR1/S;700;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x450 UR1/S;700;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x500 UR1/S;700;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x525 UR1/S;700;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 700x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 700x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x50 UR1/S;725;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x75 UR1/S;725;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x100 UR1/S;725;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x125 UR1/S;725;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x150 UR1/S;725;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x200 UR1/S;725;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x225 UR1/S;725;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x250 UR1/S;725;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x300 UR1/S;725;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x325 UR1/S;725;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x350 UR1/S;725;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x400 UR1/S;725;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x425 UR1/S;725;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x450 UR1/S;725;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x500 UR1/S;725;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x525 UR1/S;725;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 725x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 725x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x50 UR1/S;800;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x75 UR1/S;800;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x100 UR1/S;800;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x125 UR1/S;800;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x150 UR1/S;800;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x200 UR1/S;800;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x225 UR1/S;800;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x250 UR1/S;800;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x300 UR1/S;800;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x325 UR1/S;800;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x350 UR1/S;800;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x400 UR1/S;800;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x425 UR1/S;800;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x450 UR1/S;800;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x500 UR1/S;800;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x525 UR1/S;800;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 800x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 800x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x50 UR1/S;825;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x75 UR1/S;825;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x100 UR1/S;825;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x125 UR1/S;825;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x150 UR1/S;825;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x200 UR1/S;825;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x225 UR1/S;825;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x250 UR1/S;825;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x300 UR1/S;825;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x325 UR1/S;825;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x350 UR1/S;825;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x400 UR1/S;825;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x425 UR1/S;825;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x450 UR1/S;825;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x500 UR1/S;825;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x525 UR1/S;825;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 825x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 825x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x50 UR1/S;1000;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x75 UR1/S;1000;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x100 UR1/S;1000;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x125 UR1/S;1000;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x150 UR1/S;1000;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x200 UR1/S;1000;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x225 UR1/S;1000;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x250 UR1/S;1000;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x300 UR1/S;1000;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x325 UR1/S;1000;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x350 UR1/S;1000;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x400 UR1/S;1000;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x425 UR1/S;1000;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x450 UR1/S;1000;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x500 UR1/S;1000;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x525 UR1/S;1000;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1000x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x50 UR1/S;1025;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x75 UR1/S;1025;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x100 UR1/S;1025;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x125 UR1/S;1025;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x150 UR1/S;1025;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x200 UR1/S;1025;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x225 UR1/S;1025;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x250 UR1/S;1025;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x300 UR1/S;1025;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x325 UR1/S;1025;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x350 UR1/S;1025;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x400 UR1/S;1025;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x425 UR1/S;1025;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x450 UR1/S;1025;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x500 UR1/S;1025;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x525 UR1/S;1025;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1025x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x50 UR1/S;1225;50;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x50, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x50 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x75 UR1/S;1225;75;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x75, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x75 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x100 UR1/S;1225;100;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x100, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x100 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x125 UR1/S;1225;125;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x125, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x125 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x150 UR1/S;1225;150;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x150, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x150 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x200 UR1/S;1225;200;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x200, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x200 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x225 UR1/S;1225;225;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x225, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x225 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x250 UR1/S;1225;250;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x250, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x250 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x300 UR1/S;1225;300;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x300, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x300 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x325 UR1/S;1225;325;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x325, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x325 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x350 UR1/S;1225;350;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x350, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x350 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x400 UR1/S;1225;400;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x400, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x400 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x425 UR1/S;1225;425;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x425, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x425 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x450 UR1/S;1225;450;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x450, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x450 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x500 UR1/S;1225;500;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x500, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x500 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x525 UR1/S;1225;525;20;UR1;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x525, mounting frame with holders for threaded rods, screw fastening;MANDÍK;SMM 20 1225x525 UR1/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x50 UR2/S;200;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x75 UR2/S;200;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x100 UR2/S;200;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x125 UR2/S;200;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x150 UR2/S;200;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x200 UR2/S;200;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x225 UR2/S;200;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x250 UR2/S;200;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x300 UR2/S;200;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x325 UR2/S;200;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x350 UR2/S;200;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x400 UR2/S;200;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x425 UR2/S;200;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x450 UR2/S;200;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x500 UR2/S;200;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 200x525 UR2/S;200;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 200x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 200x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x50 UR2/S;225;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x75 UR2/S;225;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x100 UR2/S;225;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x125 UR2/S;225;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x150 UR2/S;225;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x200 UR2/S;225;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x225 UR2/S;225;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x250 UR2/S;225;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x300 UR2/S;225;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x325 UR2/S;225;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x350 UR2/S;225;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x400 UR2/S;225;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x425 UR2/S;225;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x450 UR2/S;225;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x500 UR2/S;225;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 225x525 UR2/S;225;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 225x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 225x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x50 UR2/S;300;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x75 UR2/S;300;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x100 UR2/S;300;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x125 UR2/S;300;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x150 UR2/S;300;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x200 UR2/S;300;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x225 UR2/S;300;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x250 UR2/S;300;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x300 UR2/S;300;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x325 UR2/S;300;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x350 UR2/S;300;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x400 UR2/S;300;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x425 UR2/S;300;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x450 UR2/S;300;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x500 UR2/S;300;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 300x525 UR2/S;300;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 300x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 300x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x50 UR2/S;325;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x75 UR2/S;325;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x100 UR2/S;325;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x125 UR2/S;325;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x150 UR2/S;325;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x200 UR2/S;325;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x225 UR2/S;325;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x250 UR2/S;325;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x300 UR2/S;325;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x325 UR2/S;325;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x350 UR2/S;325;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x400 UR2/S;325;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x425 UR2/S;325;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x450 UR2/S;325;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x500 UR2/S;325;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 325x525 UR2/S;325;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 325x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 325x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x50 UR2/S;400;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x75 UR2/S;400;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x100 UR2/S;400;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x125 UR2/S;400;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x150 UR2/S;400;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x200 UR2/S;400;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x225 UR2/S;400;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x250 UR2/S;400;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x300 UR2/S;400;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x325 UR2/S;400;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x350 UR2/S;400;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x400 UR2/S;400;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x425 UR2/S;400;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x450 UR2/S;400;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x500 UR2/S;400;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 400x525 UR2/S;400;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 400x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 400x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x50 UR2/S;425;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x75 UR2/S;425;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x100 UR2/S;425;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x125 UR2/S;425;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x150 UR2/S;425;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x200 UR2/S;425;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x225 UR2/S;425;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x250 UR2/S;425;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x300 UR2/S;425;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x325 UR2/S;425;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x350 UR2/S;425;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x400 UR2/S;425;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x425 UR2/S;425;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x450 UR2/S;425;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x500 UR2/S;425;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 425x525 UR2/S;425;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 425x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 425x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x50 UR2/S;500;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x75 UR2/S;500;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x100 UR2/S;500;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x125 UR2/S;500;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x150 UR2/S;500;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x200 UR2/S;500;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x225 UR2/S;500;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x250 UR2/S;500;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x300 UR2/S;500;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x325 UR2/S;500;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x350 UR2/S;500;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x400 UR2/S;500;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x425 UR2/S;500;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x450 UR2/S;500;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x500 UR2/S;500;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 500x525 UR2/S;500;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 500x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 500x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x50 UR2/S;525;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x75 UR2/S;525;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x100 UR2/S;525;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x125 UR2/S;525;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x150 UR2/S;525;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x200 UR2/S;525;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x225 UR2/S;525;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x250 UR2/S;525;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x300 UR2/S;525;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x325 UR2/S;525;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x350 UR2/S;525;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x400 UR2/S;525;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x425 UR2/S;525;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x450 UR2/S;525;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x500 UR2/S;525;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 525x525 UR2/S;525;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 525x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 525x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x50 UR2/S;600;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x75 UR2/S;600;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x100 UR2/S;600;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x125 UR2/S;600;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x150 UR2/S;600;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x200 UR2/S;600;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x225 UR2/S;600;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x250 UR2/S;600;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x300 UR2/S;600;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x325 UR2/S;600;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x350 UR2/S;600;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x400 UR2/S;600;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x425 UR2/S;600;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x450 UR2/S;600;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x500 UR2/S;600;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 600x525 UR2/S;600;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 600x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 600x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x50 UR2/S;625;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x75 UR2/S;625;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x100 UR2/S;625;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x125 UR2/S;625;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x150 UR2/S;625;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x200 UR2/S;625;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x225 UR2/S;625;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x250 UR2/S;625;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x300 UR2/S;625;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x325 UR2/S;625;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x350 UR2/S;625;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x400 UR2/S;625;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x425 UR2/S;625;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x450 UR2/S;625;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x500 UR2/S;625;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 625x525 UR2/S;625;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 625x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 625x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x50 UR2/S;700;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x75 UR2/S;700;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x100 UR2/S;700;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x125 UR2/S;700;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x150 UR2/S;700;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x200 UR2/S;700;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x225 UR2/S;700;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x250 UR2/S;700;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x300 UR2/S;700;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x325 UR2/S;700;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x350 UR2/S;700;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x400 UR2/S;700;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x425 UR2/S;700;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x450 UR2/S;700;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x500 UR2/S;700;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 700x525 UR2/S;700;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 700x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 700x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x50 UR2/S;725;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x75 UR2/S;725;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x100 UR2/S;725;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x125 UR2/S;725;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x150 UR2/S;725;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x200 UR2/S;725;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x225 UR2/S;725;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x250 UR2/S;725;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x300 UR2/S;725;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x325 UR2/S;725;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x350 UR2/S;725;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x400 UR2/S;725;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x425 UR2/S;725;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x450 UR2/S;725;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x500 UR2/S;725;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 725x525 UR2/S;725;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 725x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 725x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x50 UR2/S;800;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x75 UR2/S;800;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x100 UR2/S;800;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x125 UR2/S;800;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x150 UR2/S;800;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x200 UR2/S;800;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x225 UR2/S;800;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x250 UR2/S;800;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x300 UR2/S;800;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x325 UR2/S;800;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x350 UR2/S;800;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x400 UR2/S;800;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x425 UR2/S;800;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x450 UR2/S;800;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x500 UR2/S;800;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 800x525 UR2/S;800;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 800x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 800x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x50 UR2/S;825;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x75 UR2/S;825;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x100 UR2/S;825;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x125 UR2/S;825;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x150 UR2/S;825;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x200 UR2/S;825;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x225 UR2/S;825;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x250 UR2/S;825;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x300 UR2/S;825;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x325 UR2/S;825;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x350 UR2/S;825;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x400 UR2/S;825;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x425 UR2/S;825;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x450 UR2/S;825;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x500 UR2/S;825;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 825x525 UR2/S;825;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 825x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 825x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x50 UR2/S;1000;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x75 UR2/S;1000;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x100 UR2/S;1000;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x125 UR2/S;1000;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x150 UR2/S;1000;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x200 UR2/S;1000;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x225 UR2/S;1000;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x250 UR2/S;1000;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x300 UR2/S;1000;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x325 UR2/S;1000;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x350 UR2/S;1000;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x400 UR2/S;1000;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x425 UR2/S;1000;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x450 UR2/S;1000;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x500 UR2/S;1000;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1000x525 UR2/S;1000;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1000x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1000x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x50 UR2/S;1025;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x75 UR2/S;1025;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x100 UR2/S;1025;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x125 UR2/S;1025;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x150 UR2/S;1025;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x200 UR2/S;1025;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x225 UR2/S;1025;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x250 UR2/S;1025;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x300 UR2/S;1025;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x325 UR2/S;1025;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x350 UR2/S;1025;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x400 UR2/S;1025;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x425 UR2/S;1025;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x450 UR2/S;1025;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x500 UR2/S;1025;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1025x525 UR2/S;1025;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1025x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1025x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x50 UR2/S;1225;50;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x75 UR2/S;1225;75;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x100 UR2/S;1225;100;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x125 UR2/S;1225;125;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x150 UR2/S;1225;150;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x200 UR2/S;1225;200;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x225 UR2/S;1225;225;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x250 UR2/S;1225;250;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x300 UR2/S;1225;300;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x325 UR2/S;1225;325;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x350 UR2/S;1225;350;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x400 UR2/S;1225;400;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x425 UR2/S;1225;425;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x450 UR2/S;1225;450;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x500 UR2/S;1225;500;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 12,5 1225x525 UR2/S;1225;525;12,5;UR2;Wall mounted grilles;slats spacing 12,5, nominal dimensions 1225x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 12,5 1225x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x50 UR2/S;200;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x75 UR2/S;200;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x100 UR2/S;200;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x125 UR2/S;200;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x150 UR2/S;200;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x200 UR2/S;200;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x225 UR2/S;200;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x250 UR2/S;200;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x300 UR2/S;200;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x325 UR2/S;200;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x350 UR2/S;200;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x400 UR2/S;200;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x425 UR2/S;200;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x450 UR2/S;200;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x500 UR2/S;200;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 200x525 UR2/S;200;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 200x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 200x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x50 UR2/S;225;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x75 UR2/S;225;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x100 UR2/S;225;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x125 UR2/S;225;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x150 UR2/S;225;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x200 UR2/S;225;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x225 UR2/S;225;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x250 UR2/S;225;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x300 UR2/S;225;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x325 UR2/S;225;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x350 UR2/S;225;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x400 UR2/S;225;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x425 UR2/S;225;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x450 UR2/S;225;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x500 UR2/S;225;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 225x525 UR2/S;225;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 225x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 225x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x50 UR2/S;300;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x75 UR2/S;300;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x100 UR2/S;300;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x125 UR2/S;300;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x150 UR2/S;300;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x200 UR2/S;300;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x225 UR2/S;300;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x250 UR2/S;300;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x300 UR2/S;300;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x325 UR2/S;300;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x350 UR2/S;300;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x400 UR2/S;300;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x425 UR2/S;300;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x450 UR2/S;300;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x500 UR2/S;300;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 300x525 UR2/S;300;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 300x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 300x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x50 UR2/S;325;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x75 UR2/S;325;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x100 UR2/S;325;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x125 UR2/S;325;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x150 UR2/S;325;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x200 UR2/S;325;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x225 UR2/S;325;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x250 UR2/S;325;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x300 UR2/S;325;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x325 UR2/S;325;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x350 UR2/S;325;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x400 UR2/S;325;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x425 UR2/S;325;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x450 UR2/S;325;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x500 UR2/S;325;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 325x525 UR2/S;325;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 325x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 325x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x50 UR2/S;400;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x75 UR2/S;400;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x100 UR2/S;400;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x125 UR2/S;400;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x150 UR2/S;400;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x200 UR2/S;400;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x225 UR2/S;400;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x250 UR2/S;400;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x300 UR2/S;400;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x325 UR2/S;400;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x350 UR2/S;400;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x400 UR2/S;400;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x425 UR2/S;400;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x450 UR2/S;400;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x500 UR2/S;400;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 400x525 UR2/S;400;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 400x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 400x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x50 UR2/S;425;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x75 UR2/S;425;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x100 UR2/S;425;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x125 UR2/S;425;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x150 UR2/S;425;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x200 UR2/S;425;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x225 UR2/S;425;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x250 UR2/S;425;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x300 UR2/S;425;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x325 UR2/S;425;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x350 UR2/S;425;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x400 UR2/S;425;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x425 UR2/S;425;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x450 UR2/S;425;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x500 UR2/S;425;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 425x525 UR2/S;425;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 425x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 425x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x50 UR2/S;500;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x75 UR2/S;500;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x100 UR2/S;500;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x125 UR2/S;500;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x150 UR2/S;500;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x200 UR2/S;500;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x225 UR2/S;500;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x250 UR2/S;500;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x300 UR2/S;500;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x325 UR2/S;500;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x350 UR2/S;500;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x400 UR2/S;500;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x425 UR2/S;500;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x450 UR2/S;500;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x500 UR2/S;500;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 500x525 UR2/S;500;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 500x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 500x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x50 UR2/S;525;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x75 UR2/S;525;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x100 UR2/S;525;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x125 UR2/S;525;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x150 UR2/S;525;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x200 UR2/S;525;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x225 UR2/S;525;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x250 UR2/S;525;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x300 UR2/S;525;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x325 UR2/S;525;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x350 UR2/S;525;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x400 UR2/S;525;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x425 UR2/S;525;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x450 UR2/S;525;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x500 UR2/S;525;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 525x525 UR2/S;525;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 525x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 525x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x50 UR2/S;600;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x75 UR2/S;600;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x100 UR2/S;600;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x125 UR2/S;600;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x150 UR2/S;600;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x200 UR2/S;600;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x225 UR2/S;600;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x250 UR2/S;600;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x300 UR2/S;600;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x325 UR2/S;600;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x350 UR2/S;600;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x400 UR2/S;600;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x425 UR2/S;600;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x450 UR2/S;600;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x500 UR2/S;600;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 600x525 UR2/S;600;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 600x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 600x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x50 UR2/S;625;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x75 UR2/S;625;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x100 UR2/S;625;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x125 UR2/S;625;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x150 UR2/S;625;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x200 UR2/S;625;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x225 UR2/S;625;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x250 UR2/S;625;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x300 UR2/S;625;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x325 UR2/S;625;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x350 UR2/S;625;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x400 UR2/S;625;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x425 UR2/S;625;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x450 UR2/S;625;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x500 UR2/S;625;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 625x525 UR2/S;625;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 625x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 625x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x50 UR2/S;700;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x75 UR2/S;700;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x100 UR2/S;700;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x125 UR2/S;700;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x150 UR2/S;700;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x200 UR2/S;700;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x225 UR2/S;700;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x250 UR2/S;700;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x300 UR2/S;700;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x325 UR2/S;700;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x350 UR2/S;700;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x400 UR2/S;700;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x425 UR2/S;700;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x450 UR2/S;700;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x500 UR2/S;700;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 700x525 UR2/S;700;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 700x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 700x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x50 UR2/S;725;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x75 UR2/S;725;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x100 UR2/S;725;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x125 UR2/S;725;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x150 UR2/S;725;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x200 UR2/S;725;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x225 UR2/S;725;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x250 UR2/S;725;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x300 UR2/S;725;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x325 UR2/S;725;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x350 UR2/S;725;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x400 UR2/S;725;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x425 UR2/S;725;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x450 UR2/S;725;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x500 UR2/S;725;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 725x525 UR2/S;725;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 725x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 725x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x50 UR2/S;800;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x75 UR2/S;800;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x100 UR2/S;800;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x125 UR2/S;800;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x150 UR2/S;800;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x200 UR2/S;800;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x225 UR2/S;800;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x250 UR2/S;800;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x300 UR2/S;800;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x325 UR2/S;800;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x350 UR2/S;800;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x400 UR2/S;800;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x425 UR2/S;800;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x450 UR2/S;800;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x500 UR2/S;800;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 800x525 UR2/S;800;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 800x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 800x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x50 UR2/S;825;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x75 UR2/S;825;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x100 UR2/S;825;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x125 UR2/S;825;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x150 UR2/S;825;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x200 UR2/S;825;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x225 UR2/S;825;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x250 UR2/S;825;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x300 UR2/S;825;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x325 UR2/S;825;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x350 UR2/S;825;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x400 UR2/S;825;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x425 UR2/S;825;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x450 UR2/S;825;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x500 UR2/S;825;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 825x525 UR2/S;825;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 825x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 825x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x50 UR2/S;1000;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x75 UR2/S;1000;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x100 UR2/S;1000;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x125 UR2/S;1000;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x150 UR2/S;1000;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x200 UR2/S;1000;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x225 UR2/S;1000;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x250 UR2/S;1000;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x300 UR2/S;1000;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x325 UR2/S;1000;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x350 UR2/S;1000;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x400 UR2/S;1000;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x425 UR2/S;1000;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x450 UR2/S;1000;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x500 UR2/S;1000;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1000x525 UR2/S;1000;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1000x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1000x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x50 UR2/S;1025;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x75 UR2/S;1025;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x100 UR2/S;1025;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x125 UR2/S;1025;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x150 UR2/S;1025;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x200 UR2/S;1025;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x225 UR2/S;1025;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x250 UR2/S;1025;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x300 UR2/S;1025;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x325 UR2/S;1025;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x350 UR2/S;1025;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x400 UR2/S;1025;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x425 UR2/S;1025;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x450 UR2/S;1025;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x500 UR2/S;1025;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1025x525 UR2/S;1025;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1025x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1025x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x50 UR2/S;1225;50;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x50, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x50 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x75 UR2/S;1225;75;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x75, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x75 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x100 UR2/S;1225;100;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x100, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x100 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x125 UR2/S;1225;125;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x125, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x125 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x150 UR2/S;1225;150;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x150, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x150 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x200 UR2/S;1225;200;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x200, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x200 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x225 UR2/S;1225;225;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x225, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x225 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x250 UR2/S;1225;250;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x250, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x250 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x300 UR2/S;1225;300;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x300, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x300 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x325 UR2/S;1225;325;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x325, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x325 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x350 UR2/S;1225;350;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x350, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x350 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x400 UR2/S;1225;400;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x400, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x400 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x425 UR2/S;1225;425;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x425, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x425 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x450 UR2/S;1225;450;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x450, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x450 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x500 UR2/S;1225;500;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x500, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x500 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
SMM 20 1225x525 UR2/S;1225;525;20;UR2;Wall mounted grilles;slats spacing 20, nominal dimensions 1225x525, mounting frame with wall brackets, screw fastening;MANDÍK;SMM 20 1225x525 UR2/S;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/smm
