;DUCT_DIAMETER##HVAC_DUCT_SIZE##MILLIMETERS;Height of the box##LENGTH##MILLIMETERS;Width of the box##LENGTH##MILLIMETERS;Length of the box##LENGTH##MILLIMETERS;Number of slots##OTHER##;Number of nozzles##OTHER##;Description##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;Model##OTHER##;URL##OTHER##
SDL 1 500 R/P;160;235;73;500;1;1;Outlet;linear slot diffuser, number of slot outlets - 1, diffuser length 500, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 500 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 600 R/P;160;235;73;600;1;1;Outlet;linear slot diffuser, number of slot outlets - 1, diffuser length 600, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 600 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 700 R/P;160;235;73;700;1;1;Outlet;linear slot diffuser, number of slot outlets - 1, diffuser length 700, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 700 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 800 R/P;160;235;73;800;1;1;Outlet;linear slot diffuser, number of slot outlets - 1, diffuser length 800, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 800 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 900 R/P;160;235;73;900;1;1;Outlet;linear slot diffuser, number of slot outlets - 1, diffuser length 900, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 900 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 500 R/P;160;235;113;500;2;1;Outlet;linear slot diffuser, number of slot outlets - 2, diffuser length 500, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 500 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 600 R/P;160;235;113;600;2;1;Outlet;linear slot diffuser, number of slot outlets - 2, diffuser length 600, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 600 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 700 R/P;160;235;113;700;2;1;Outlet;linear slot diffuser, number of slot outlets - 2, diffuser length 700, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 700 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 800 R/P;160;235;113;800;2;1;Outlet;linear slot diffuser, number of slot outlets - 2, diffuser length 800, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 800 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 900 R/P;160;235;113;900;2;1;Outlet;linear slot diffuser, number of slot outlets - 2, diffuser length 900, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 900 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 500 R/P;200;275;152;500;3;1;Outlet;linear slot diffuser, number of slot outlets - 3, diffuser length 500, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 500 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 600 R/P;200;275;152;600;3;1;Outlet;linear slot diffuser, number of slot outlets - 3, diffuser length 600, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 600 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 700 R/P;200;275;152;700;3;1;Outlet;linear slot diffuser, number of slot outlets - 3, diffuser length 700, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 700 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 800 R/P;200;275;152;800;3;1;Outlet;linear slot diffuser, number of slot outlets - 3, diffuser length 800, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 800 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 900 R/P;200;275;152;900;3;1;Outlet;linear slot diffuser, number of slot outlets - 3, diffuser length 900, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 900 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 500 R/P;200;275;192;500;4;1;Outlet;linear slot diffuser, number of slot outlets - 4, diffuser length 500, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 500 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 600 R/P;200;275;192;600;4;1;Outlet;linear slot diffuser, number of slot outlets - 4, diffuser length 600, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 600 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 700 R/P;200;275;192;700;4;1;Outlet;linear slot diffuser, number of slot outlets - 4, diffuser length 700, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 700 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 800 R/P;200;275;192;800;4;1;Outlet;linear slot diffuser, number of slot outlets - 4, diffuser length 800, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 800 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 900 R/P;200;275;192;900;4;1;Outlet;linear slot diffuser, number of slot outlets - 4, diffuser length 900, with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 900 R/P;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 500 D;160;235;73;500;1;1;Outlet;linear slot diffuser, number of slot outlets - 1, diffuser length 500, sole front plate;MANDÍK;SDL 1 500 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 600 D;160;235;73;600;1;1;Outlet;linear slot diffuser, number of slot outlets - 1, diffuser length 600, sole front plate;MANDÍK;SDL 1 600 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 700 D;160;235;73;700;1;1;Outlet;linear slot diffuser, number of slot outlets - 1, diffuser length 700, sole front plate;MANDÍK;SDL 1 700 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 800 D;160;235;73;800;1;1;Outlet;linear slot diffuser, number of slot outlets - 1, diffuser length 800, sole front plate;MANDÍK;SDL 1 800 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 900 D;160;235;73;900;1;1;Outlet;linear slot diffuser, number of slot outlets - 1, diffuser length 900, sole front plate;MANDÍK;SDL 1 900 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 500 D;160;235;113;500;2;1;Outlet;linear slot diffuser, number of slot outlets - 2, diffuser length 500, sole front plate;MANDÍK;SDL 2 500 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 600 D;160;235;113;600;2;1;Outlet;linear slot diffuser, number of slot outlets - 2, diffuser length 600, sole front plate;MANDÍK;SDL 2 600 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 700 D;160;235;113;700;2;1;Outlet;linear slot diffuser, number of slot outlets - 2, diffuser length 700, sole front plate;MANDÍK;SDL 2 700 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 800 D;160;235;113;800;2;1;Outlet;linear slot diffuser, number of slot outlets - 2, diffuser length 800, sole front plate;MANDÍK;SDL 2 800 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 900 D;160;235;113;900;2;1;Outlet;linear slot diffuser, number of slot outlets - 2, diffuser length 900, sole front plate;MANDÍK;SDL 2 900 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 500 D;200;275;152;500;3;1;Outlet;linear slot diffuser, number of slot outlets - 3, diffuser length 500, sole front plate;MANDÍK;SDL 3 500 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 600 D;200;275;152;600;3;1;Outlet;linear slot diffuser, number of slot outlets - 3, diffuser length 600, sole front plate;MANDÍK;SDL 3 600 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 700 D;200;275;152;700;3;1;Outlet;linear slot diffuser, number of slot outlets - 3, diffuser length 700, sole front plate;MANDÍK;SDL 3 700 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 800 D;200;275;152;800;3;1;Outlet;linear slot diffuser, number of slot outlets - 3, diffuser length 800, sole front plate;MANDÍK;SDL 3 800 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 900 D;200;275;152;900;3;1;Outlet;linear slot diffuser, number of slot outlets - 3, diffuser length 900, sole front plate;MANDÍK;SDL 3 900 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 500 D;200;275;192;500;4;1;Outlet;linear slot diffuser, number of slot outlets - 4, diffuser length 500, sole front plate;MANDÍK;SDL 4 500 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 600 D;200;275;192;600;4;1;Outlet;linear slot diffuser, number of slot outlets - 4, diffuser length 600, sole front plate;MANDÍK;SDL 4 600 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 700 D;200;275;192;700;4;1;Outlet;linear slot diffuser, number of slot outlets - 4, diffuser length 700, sole front plate;MANDÍK;SDL 4 700 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 800 D;200;275;192;800;4;1;Outlet;linear slot diffuser, number of slot outlets - 4, diffuser length 800, sole front plate;MANDÍK;SDL 4 800 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 900 D;200;275;192;900;4;1;Outlet;linear slot diffuser, number of slot outlets - 4, diffuser length 900, sole front plate;MANDÍK;SDL 4 900 D;http://wwhttps://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
