;DUCT_DIAMETER##HVAC_DUCT_SIZE##MILLIMETERS;Height of the box##LENGTH##MILLIMETERS;Width of the box##LENGTH##MILLIMETERS;Length of the box##LENGTH##MILLIMETERS;Number of slots##OTHER##;Number of nozzles##OTHER##;Description##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;Model##OTHER##;URL##OTHER##
SDL 1 1000 R/P;160;235;73;1000;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1000,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 1000 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1100 R/P;160;235;73;1100;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1100,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 1100 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1200 R/P;160;235;73;1200;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1200,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 1200 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1300 R/P;160;235;73;1300;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1300,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 1300 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1400 R/P;160;235;73;1400;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1400,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 1400 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1500 R/P;160;235;73;1500;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1500,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 1500 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1600 R/P;160;235;73;1600;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1600,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 1600 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1700 R/P;160;235;73;1700;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1700,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 1700 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1800 R/P;160;235;73;1800;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1800,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 1800 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1900 R/P;160;235;73;1900;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1900,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 1900 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 2000 R/P;160;235;73;2000;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 2000,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 1 2000 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1000 R/P;160;235;113;1000;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1000,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 1000 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1100 R/P;160;235;113;1100;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1100,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 1100 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1200 R/P;160;235;113;1200;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1200,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 1200 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1300 R/P;160;235;113;1300;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1300,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 1300 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1400 R/P;160;235;113;1400;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1400,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 1400 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1500 R/P;160;235;113;1500;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1500,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 1500 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1600 R/P;160;235;113;1600;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1600,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 1600 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1700 R/P;160;235;113;1700;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1700,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 1700 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1800 R/P;160;235;113;1800;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1800,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 1800 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1900 R/P;160;235;113;1900;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1900,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 1900 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 2000 R/P;160;235;113;2000;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 2000,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 2 2000 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1000 R/P;200;275;152;1000;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1000,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 1000 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1100 R/P;200;275;152;1100;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1100,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 1100 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1200 R/P;200;275;152;1200;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1200,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 1200 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1300 R/P;200;275;152;1300;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1300,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 1300 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1400 R/P;200;275;152;1400;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1400,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 1400 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1500 R/P;200;275;152;1500;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1500,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 1500 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1600 R/P;200;275;152;1600;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1600,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 1600 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1700 R/P;200;275;152;1700;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1700,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 1700 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1800 R/P;200;275;152;1800;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1800,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 1800 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1900 R/P;200;275;152;1900;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1900,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 1900 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 2000 R/P;200;275;152;2000;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 2000,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 3 2000 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1000 R/P;200;275;192;1000;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1000,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 1000 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1100 R/P;200;275;192;1100;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1100,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 1100 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1200 R/P;200;275;192;1200;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1200,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 1200 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1300 R/P;200;275;192;1300;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1300,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 1300 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1400 R/P;200;275;192;1400;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1400,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 1400 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1500 R/P;200;275;192;1500;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1500,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 1500 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1600 R/P;200;275;192;1600;4;3;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1600,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 1600 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1700 R/P;200;275;192;1700;4;3;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1700,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 1700 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1800 R/P;200;275;192;1800;4;3;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1800,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 1800 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1900 R/P;200;275;192;1900;4;3;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1900,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 1900 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 2000 R/P;200;275;192;2000;4;3;Outlet;linear slot diffuser, number of slots - 4, diffuser length 2000,  with a control flap in nozzle, covered front plate fixation;MANDÍK;SDL 4 2000 R/P;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1000 D;160;235;73;1000;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1000, sole front plate;MANDÍK;SDL 1 1000 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1100 D;160;235;73;1100;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1100, sole front plate;MANDÍK;SDL 1 1100 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1200 D;160;235;73;1200;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1200, sole front plate;MANDÍK;SDL 1 1200 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1300 D;160;235;73;1300;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1300, sole front plate;MANDÍK;SDL 1 1300 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1400 D;160;235;73;1400;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1400, sole front plate;MANDÍK;SDL 1 1400 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1500 D;160;235;73;1500;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1500, sole front plate;MANDÍK;SDL 1 1500 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1600 D;160;235;73;1600;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1600, sole front plate;MANDÍK;SDL 1 1600 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1700 D;160;235;73;1700;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1700, sole front plate;MANDÍK;SDL 1 1700 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1800 D;160;235;73;1800;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1800, sole front plate;MANDÍK;SDL 1 1800 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 1900 D;160;235;73;1900;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 1900, sole front plate;MANDÍK;SDL 1 1900 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 1 2000 D;160;235;73;2000;1;2;Outlet;linear slot diffuser, number of slots - 1, diffuser length 2000, sole front plate;MANDÍK;SDL 1 2000 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1000 D;160;235;113;1000;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1000, sole front plate;MANDÍK;SDL 2 1000 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1100 D;160;235;113;1100;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1100, sole front plate;MANDÍK;SDL 2 1100 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1200 D;160;235;113;1200;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1200, sole front plate;MANDÍK;SDL 2 1200 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1300 D;160;235;113;1300;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1300, sole front plate;MANDÍK;SDL 2 1300 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1400 D;160;235;113;1400;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1400, sole front plate;MANDÍK;SDL 2 1400 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1500 D;160;235;113;1500;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1500, sole front plate;MANDÍK;SDL 2 1500 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1600 D;160;235;113;1600;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1600, sole front plate;MANDÍK;SDL 2 1600 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1700 D;160;235;113;1700;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1700, sole front plate;MANDÍK;SDL 2 1700 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1800 D;160;235;113;1800;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1800, sole front plate;MANDÍK;SDL 2 1800 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 1900 D;160;235;113;1900;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 1900, sole front plate;MANDÍK;SDL 2 1900 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 2 2000 D;160;235;113;2000;2;2;Outlet;linear slot diffuser, number of slots - 2, diffuser length 2000, sole front plate;MANDÍK;SDL 2 2000 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1000 D;200;275;152;1000;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1000, sole front plate;MANDÍK;SDL 3 1000 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1100 D;200;275;152;1100;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1100, sole front plate;MANDÍK;SDL 3 1100 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1200 D;200;275;152;1200;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1200, sole front plate;MANDÍK;SDL 3 1200 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1300 D;200;275;152;1300;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1300, sole front plate;MANDÍK;SDL 3 1300 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1400 D;200;275;152;1400;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1400, sole front plate;MANDÍK;SDL 3 1400 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1500 D;200;275;152;1500;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1500, sole front plate;MANDÍK;SDL 3 1500 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1600 D;200;275;152;1600;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1600, sole front plate;MANDÍK;SDL 3 1600 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1700 D;200;275;152;1700;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1700, sole front plate;MANDÍK;SDL 3 1700 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1800 D;200;275;152;1800;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1800, sole front plate;MANDÍK;SDL 3 1800 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 1900 D;200;275;152;1900;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 1900, sole front plate;MANDÍK;SDL 3 1900 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 3 2000 D;200;275;152;2000;3;2;Outlet;linear slot diffuser, number of slots - 3, diffuser length 2000, sole front plate;MANDÍK;SDL 3 2000 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1000 D;200;275;192;1000;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1000, sole front plate;MANDÍK;SDL 4 1000 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1100 D;200;275;192;1100;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1100, sole front plate;MANDÍK;SDL 4 1100 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1200 D;200;275;192;1200;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1200, sole front plate;MANDÍK;SDL 4 1200 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1300 D;200;275;192;1300;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1300, sole front plate;MANDÍK;SDL 4 1300 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1400 D;200;275;192;1400;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1400, sole front plate;MANDÍK;SDL 4 1400 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1500 D;200;275;192;1500;4;2;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1500, sole front plate;MANDÍK;SDL 4 1500 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1600 D;200;275;192;1600;4;3;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1600, sole front plate;MANDÍK;SDL 4 1600 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1700 D;200;275;192;1700;4;3;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1700, sole front plate;MANDÍK;SDL 4 1700 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1800 D;200;275;192;1800;4;3;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1800, sole front plate;MANDÍK;SDL 4 1800 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 1900 D;200;275;192;1900;4;3;Outlet;linear slot diffuser, number of slots - 4, diffuser length 1900, sole front plate;MANDÍK;SDL 4 1900 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
SDL 4 2000 D;200;275;192;2000;4;3;Outlet;linear slot diffuser, number of slots - 4, diffuser length 2000, sole front plate;MANDÍK;SDL 4 2000 D;https://www.mandik.cz/product-line/distribution-elements/grilles-and-vents/sdl
